(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "RaspberryPi_Pico"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -19.05 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "RaspberryPi_Pico"
			(at 7.62 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_Common"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Versatile and inexpensive microcontroller module powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico microcontroller module RP2040 M0+ usb"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?Common* RaspberryPi?Pico?Original*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "RaspberryPi_Pico_0_1"
			(rectangle
				(start -19.05 36.83)
				(end 19.05 -34.29)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 0 36.83) (xy 1.27 36.195) (xy 1.27 34.29) (xy 1.905 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 34.29) (xy 3.175 35.56) (xy 3.175 33.02) (xy 1.905 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 36.83) (xy 3.81 36.195) (xy 3.81 34.29) (xy 3.175 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -34.29) (xy 1.27 -33.655) (xy 1.27 -21.59) (xy 18.415 -21.59) (xy 19.05 -20.32)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.651 35.306) (xy 1.651 35.56) (xy 1.905 35.56) (xy 1.905 33.02) (xy 2.159 33.02) (xy 2.159 33.274)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "RaspberryPi_Pico_1_1"
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "GPIO0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "GPIO7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM3_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "GPIO8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM4_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "GPIO9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM4_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "GPIO10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "GPIO11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "GPIO12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "GPIO13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM6_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "GPIO14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM7_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "GPIO1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" passive line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "GPIO15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM7_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "GPIO16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "GPIO17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "GPIO18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "GPIO19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "GPIO20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPIN0" input clock)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "GPIO21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPOUT0" output clock)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "GPIO22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPIN1" input clock)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_out line
				(at 0 -38.1 90)
				(length 3.81)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "GND_IN" power_in line)
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "RUN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "~{RESET}" input line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "GPIO26_ADC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC0" input line)
				(alternate "GPIO26" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "GPIO27_ADC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1" input line)
				(alternate "GPIO27" bidirectional line)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin power_out line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "AGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "GND" passive line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "GPIO28_ADC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC2" input line)
				(alternate "GPIO28" bidirectional line)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_in line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "ADC_VREF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at -5.08 40.64 270)
				(length 3.81)
				(name "3V3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "3V3_EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "~{3V3_DISABLE}" input line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 3.81)
				(name "VSYS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VSYS_IN" power_in line)
				(alternate "VSYS_OUT" power_out line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "GPIO2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_out line
				(at 5.08 40.64 270)
				(length 3.81)
				(name "VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VBUS_HOST" power_in line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "GPIO3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "GPIO4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "GPIO5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "GPIO6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
		)
	)
	(symbol "RaspberryPi_Pico_DebugPins"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -19.05 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "RaspberryPi_Pico"
			(at 7.62 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_Original_SMD_HandSolder"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Versatile and inexpensive microcontroller module (with debug pins) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico microcontroller module RP2040 M0+ usb swd debug"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?Original?SMD*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "RaspberryPi_Pico_DebugPins_0_1"
			(rectangle
				(start -19.05 36.83)
				(end 19.05 -34.29)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 0 36.83) (xy 1.27 36.195) (xy 1.27 34.29) (xy 1.905 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 34.29) (xy 3.175 35.56) (xy 3.175 33.02) (xy 1.905 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 36.83) (xy 3.81 36.195) (xy 3.81 34.29) (xy 3.175 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -34.29) (xy 1.27 -33.655) (xy 1.27 -21.59) (xy 18.415 -21.59) (xy 19.05 -20.32)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.651 35.306) (xy 1.651 35.56) (xy 1.905 35.56) (xy 1.905 33.02) (xy 2.159 33.02) (xy 2.159 33.274)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "RaspberryPi_Pico_DebugPins_1_1"
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "GPIO0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "GPIO7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM3_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "GPIO8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM4_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "GPIO9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM4_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "GPIO10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "GPIO11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "GPIO12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "GPIO13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM6_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "GPIO14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM7_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "GPIO1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" passive line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "GPIO15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM7_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "GPIO16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "GPIO17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "GPIO18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "GPIO19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "GPIO20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPIN0" input clock)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "GPIO21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPOUT0" output clock)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "GPIO22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPIN1" input clock)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_out line
				(at 0 -38.1 90)
				(length 3.81)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "GND_IN" power_in line)
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "RUN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "~{RESET}" input line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "GPIO26_ADC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC0" input line)
				(alternate "GPIO26" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "GPIO27_ADC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1" input line)
				(alternate "GPIO27" bidirectional line)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin power_out line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "AGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "GND" passive line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "GPIO28_ADC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC2" input line)
				(alternate "GPIO28" bidirectional line)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_in line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "ADC_VREF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at -5.08 40.64 270)
				(length 3.81)
				(name "3V3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "3V3_EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "~{3V3_DISABLE}" input line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 3.81)
				(name "VSYS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VSYS_IN" power_in line)
				(alternate "VSYS_OUT" power_out line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "GPIO2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_out line
				(at 5.08 40.64 270)
				(length 3.81)
				(name "VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VBUS_HOST" power_in line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "GPIO3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "GPIO4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "GPIO5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "GPIO6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "D1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "D2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "D3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "RaspberryPi_Pico_InternalPullUp-3V3_EN"
		(pin_numbers hide)
		(pin_names hide)
		(exclude_from_sim no)
		(in_bom no)
		(on_board no)
		(property "Reference" "#INT"
			(at 0 -7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "InternalPullUp_3V3_EN"
			(at 0 -5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -10.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Symbol for the internal pull-up resistor on the Raspberry Pi Pico 3V3_EN pin, to make ERC happy when connecting to open collectors"
			(at 0 -12.7 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico internal pull up pull-up resistor erc rule rules"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "RaspberryPi_Pico_InternalPullUp-3V3_EN_0_1"
			(polyline
				(pts
					(xy 8.89 -2.54) (xy 12.065 -2.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 5.715 -1.905)
				(end 8.89 -3.175)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "RaspberryPi_Pico_InternalPullUp-3V3_EN_1_1"
			(polyline
				(pts
					(xy 5.715 -2.54) (xy 5.08 -2.54) (xy 3.81 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(text "100k"
				(at 7.3025 -2.54 0)
				(effects
					(font
						(size 0.635 0.635)
					)
				)
			)
			(text "VSYS"
				(at 12.065 -1.905 0)
				(effects
					(font
						(size 0.635 0.635)
					)
					(justify right)
				)
			)
			(pin passive line
				(at 0 0 0)
				(length 3.81)
				(name "INTERNAL_PULL_UP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "RaspberryPi_Pico_MultiPart-Module"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at 7.62 40.64 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "RaspberryPi_Pico"
			(at 7.62 38.1 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_Original_Virtual"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Versatile and inexpensive microcontroller module powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico microcontroller module RP2040 M0+ usb virtual"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?Original?Virtual*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "RaspberryPi_Pico_MultiPart-Module_0_1"
			(polyline
				(pts
					(xy 0 36.83) (xy 1.27 36.195) (xy 1.27 34.29) (xy 1.905 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 34.29) (xy 3.175 35.56) (xy 3.175 33.02) (xy 1.905 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 36.83) (xy 3.81 36.195) (xy 3.81 34.29) (xy 3.175 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -34.29) (xy 1.27 -33.655) (xy 1.27 -21.59) (xy 18.415 -21.59) (xy 19.05 -20.32)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.651 35.306) (xy 1.651 35.56) (xy 1.905 35.56) (xy 1.905 33.02) (xy 2.159 33.02) (xy 2.159 33.274)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "RaspberryPi_Pico_MultiPart-Module_1_1"
			(rectangle
				(start -19.05 36.83)
				(end 19.05 -34.29)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy -19.05 25.4) (xy -2.54 25.4) (xy -2.54 -17.78) (xy -19.05 -17.78)
				)
				(stroke
					(width 0.254)
					(type dash)
				)
				(fill
					(type none)
				)
			)
			(text "This is a virtual module meant to be paired with:\nRaspberryPi_Pico_MultiPart-Socket_A\nRaspberryPi_Pico_MultiPart-Socket_B\n\nAnd optionally with:\nRaspberryPi_Pico_MultiPart-Socket_SWD\n"
				(at 3.81 -35.56 0)
				(effects
					(font
						(size 0.762 0.762)
					)
					(justify left top)
				)
			)
		)
	)
	(symbol "RaspberryPi_Pico_MultiPart-Socket_A"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -20.32 -27.94 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Value" "Pico_Socket_A"
			(at -20.32 -30.48 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_PinSocket_1x20_P2.54mm_Vertical"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "One of two 1x20 headers for connecting a Raspberry Pi Pico, with the Pico's specific pins and capabilities implemented, single row, 01x20"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico connector socket"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*1x20*P2.54mm*Vertical*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "RaspberryPi_Pico_MultiPart-Socket_A_1_1"
			(polyline
				(pts
					(xy -19.05 25.4) (xy -19.05 -17.78)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -34.29) (xy 2.54 -34.29)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -25.4) (xy -2.54 -17.78)
				)
				(stroke
					(width 0.254)
					(type dot)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -19.05 25.4) (xy -2.54 25.4) (xy -2.54 -17.78) (xy -19.05 -17.78)
				)
				(stroke
					(width 0.254)
					(type dash)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -34.29) (xy -2.54 -25.4) (xy 2.54 -25.4) (xy 2.54 -34.29)
				)
				(stroke
					(width 0.254)
					(type dot)
				)
				(fill
					(type none)
				)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "GPIO0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "GPIO7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM3_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "GPIO8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM4_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "GPIO9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM4_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "GPIO10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "GPIO11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "GPIO12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "GPIO13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM6_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "GPIO14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM7_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "GPIO1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" passive line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "GPIO15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM7_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin power_out line
				(at 0 -38.1 90)
				(length 3.81)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "GND_IN" power_in line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "GPIO2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "GPIO3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "GPIO4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "GPIO5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "GPIO6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
		)
	)
	(symbol "RaspberryPi_Pico_MultiPart-Socket_B"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 20.32 -27.94 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "Pico_Socket_B"
			(at 20.32 -30.48 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_PinSocket_1x20_P2.54mm_Vertical"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "One of two 1x20 headers for connecting a Raspberry Pi Pico, with the Pico's specific pins and capabilities implemented, single row, 01x20"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico connector socket"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*1x20*P2.54mm*Vertical*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "RaspberryPi_Pico_MultiPart-Socket_B_1_1"
			(polyline
				(pts
					(xy -2.54 -34.29) (xy 2.54 -34.29)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -25.4) (xy -2.54 -17.78)
				)
				(stroke
					(width 0.254)
					(type dot)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -19.05 25.4) (xy -2.54 25.4) (xy -2.54 -17.78) (xy -19.05 -17.78)
				)
				(stroke
					(width 0.254)
					(type dash)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -34.29) (xy -2.54 -25.4) (xy 2.54 -25.4) (xy 2.54 -34.29)
				)
				(stroke
					(width 0.254)
					(type dot)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -19.05 -17.78) (xy -19.05 -34.29) (xy 19.05 -34.29) (xy 19.05 36.83) (xy -19.05 36.83) (xy -19.05 25.4)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "GPIO16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "RUN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "~{RESET}" input line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "GPIO26_ADC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC0" input line)
				(alternate "GPIO26" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "GPIO27_ADC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1" input line)
				(alternate "GPIO27" bidirectional line)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin power_out line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "AGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "GND" passive line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "GPIO28_ADC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC2" input line)
				(alternate "GPIO28" bidirectional line)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_in line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "ADC_VREF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at -5.08 40.64 270)
				(length 3.81)
				(name "3V3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "3V3_EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "~{3V3_DISABLE}" input line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 3.81)
				(name "VSYS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VSYS_IN" power_in line)
				(alternate "VSYS_OUT" power_out line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "GPIO17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin power_out line
				(at 5.08 40.64 270)
				(length 3.81)
				(name "VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VBUS_HOST" power_in line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "GPIO18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "GPIO19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "GPIO20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPIN0" input clock)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "GPIO21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPOUT0" output clock)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "GPIO22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPIN1" input clock)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
		)
	)
	(symbol "RaspberryPi_Pico_MultiPart-Socket_SWD"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -20.32 38.1 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Value" "Pico_SWD"
			(at -20.32 35.56 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_PinSocket_1x03_P2.54mm_Vertical"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Optional 1x03 socket for connecting a Raspberry Pi Pico's SWD pins, single row, 01x03"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico connector socket"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*1x03*P2.54mm*Vertical*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "RaspberryPi_Pico_MultiPart-Socket_SWD_1_1"
			(polyline
				(pts
					(xy -19.05 33.02) (xy -19.05 25.4)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -34.29) (xy 2.54 -34.29)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -25.4) (xy -2.54 -17.78)
				)
				(stroke
					(width 0.254)
					(type dot)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -19.05 25.4) (xy -2.54 25.4) (xy -2.54 -17.78)
				)
				(stroke
					(width 0.254)
					(type dash)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -19.05 33.02) (xy -10.795 33.02) (xy -10.795 25.4)
				)
				(stroke
					(width 0.254)
					(type dot)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -34.29) (xy -2.54 -25.4) (xy 2.54 -25.4) (xy 2.54 -34.29)
				)
				(stroke
					(width 0.254)
					(type dot)
				)
				(fill
					(type none)
				)
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "RaspberryPi_Pico_SecondaryPins"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -19.05 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "RaspberryPi_Pico"
			(at 7.62 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_Original_SMD"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Versatile and inexpensive microcontroller module (with full pinout for test point and debug connections) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico microcontroller module RP2040 M0+ usb swd debug"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?Original?SMD RaspberryPi?Pico?Original?SMD?MoutingHoles RaspberryPi?Pico?Original?SMD?MoutingHoles?HandSolder?Castellated"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "RaspberryPi_Pico_SecondaryPins_0_1"
			(rectangle
				(start -19.05 36.83)
				(end 19.05 -34.29)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 0 36.83) (xy 1.27 36.195) (xy 1.27 34.29) (xy 1.905 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 34.29) (xy 3.175 35.56) (xy 3.175 33.02) (xy 1.905 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 36.83) (xy 3.81 36.195) (xy 3.81 34.29) (xy 3.175 34.29)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -34.29) (xy 1.27 -33.655) (xy 1.27 -21.59) (xy 18.415 -21.59) (xy 19.05 -20.32)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.651 35.306) (xy 1.651 35.56) (xy 1.905 35.56) (xy 1.905 33.02) (xy 2.159 33.02) (xy 2.159 33.274)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "RaspberryPi_Pico_SecondaryPins_1_1"
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "GPIO0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "GPIO7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM3_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "GPIO8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM4_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "GPIO9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM4_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "GPIO10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "GPIO11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "GPIO12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "GPIO13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM6_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "GPIO14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM7_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "GPIO1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" passive line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "GPIO15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM7_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "GPIO16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "GPIO17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "GPIO18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "GPIO19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "GPIO20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPIN0" input clock)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "GPIO21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPOUT0" output clock)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "GPIO22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CLOCK_GPIN1" input clock)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_out line
				(at 0 -38.1 90)
				(length 3.81)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "GND_IN" power_in line)
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "RUN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "~{RESET}" input line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "GPIO26_ADC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC0" input line)
				(alternate "GPIO26" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "GPIO27_ADC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1" input line)
				(alternate "GPIO27" bidirectional line)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin power_out line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "AGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "GND" passive line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "GPIO28_ADC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC2" input line)
				(alternate "GPIO28" bidirectional line)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_in line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "ADC_VREF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at -5.08 40.64 270)
				(length 3.81)
				(name "3V3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "3V3_EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "~{3V3_DISABLE}" input line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 3.81)
				(name "VSYS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VSYS_IN" power_in line)
				(alternate "VSYS_OUT" power_out line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "GPIO2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_out line
				(at 5.08 40.64 270)
				(length 3.81)
				(name "VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VBUS_HOST" power_in line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "GPIO3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "GPIO4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "GPIO5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "GPIO6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "D1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81) hide
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "D2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "D3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "USB_GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "TP1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "USB_HOST_GND" power_in line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "USB_DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "TP2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "USB_DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "TP3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "~{SMPS_PS}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "TP4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "GPIO23_UNSAFE" output line)
				(alternate "~{SMPS_PS_UNSAFE}" output line)
			)
			(pin output line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "LED_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "TP5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "~{BOOTSEL}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "TP6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "RaspberryPi_Pico_W"
		(extends "RaspberryPi_Pico")
		(property "Reference" "A"
			(at -19.05 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "RaspberryPi_Pico_W"
			(at 7.62 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_Common"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Versatile and inexpensive wireless microcontroller module powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash, Infineon CYW43439 2.4GHz 802.11n wireless LAN"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico microcontroller module RP2040 M0+ usb CYW43439 wireless wifi bluetooth"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?Common* RaspberryPi?Pico?W*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "RaspberryPi_Pico_W_DebugPins"
		(extends "RaspberryPi_Pico_DebugPins")
		(property "Reference" "A"
			(at -19.05 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "RaspberryPi_Pico_W"
			(at 7.62 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_W_SMD"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Versatile and inexpensive wireless microcontroller module (with debug pins) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash, Infineon CYW43439 2.4GHz 802.11n wireless LAN"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico microcontroller module RP2040 M0+ usb swd debug CYW43439 wireless wifi bluetooth"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?W?SMD*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "RaspberryPi_Pico_W_MultiPart-Module"
		(extends "RaspberryPi_Pico_MultiPart-Module")
		(property "Reference" "A"
			(at 7.62 40.64 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "RaspberryPi_Pico_W"
			(at 7.62 38.1 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_W_Virtual"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Versatile and inexpensive wireless microcontroller module (virtual representation) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash, Infineon CYW43439 2.4GHz 802.11n wireless LAN"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico microcontroller module RP2040 M0+ usb CYW43439 wireless wifi bluetooth virtual"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?W?Virtual*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "RaspberryPi_Pico_W_SecondaryPins"
		(extends "RaspberryPi_Pico_SecondaryPins")
		(property "Reference" "A"
			(at -19.05 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "RaspberryPi_Pico_W"
			(at 7.62 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Module_RaspberryPi_Pico:RaspberryPi_Pico_W_SMD"
			(at 0 -49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 0 -52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Versatile and inexpensive wireless microcontroller module (with full pinout for test point and debug connections) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash, Infineon CYW43439 2.4GHz 802.11n wireless LAN"
			(at 0 -54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Raspberry Pi Pico microcontroller module RP2040 M0+ usb swd debug CYW43439 wireless wifi bluetooth"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?W?SMD RaspberryPi?Pico?W?SMD?MountingHoles RaspberryPi?Pico?W?SMD?MountingHoles?HandSolder?Castellated"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
)
