(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(uuid "0903a080-1ad6-4124-b193-44653efc0003")
		(at 35.0975 52.0225)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R6"
			(at 6.35 -2.72 0)
			(layer "F.SilkS")
			(uuid "212d0003-c88c-40ad-9372-becb697da6f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100"
			(at 6.35 2.72 0)
			(layer "F.Fab")
			(uuid "c189cc65-f987-4a26-bd42-f98d92c07713")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.koaglobal.com/-/media/Files/KOA_Global/EN/product/commonpdf/mos.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "08f79c63-fb30-41a3-87ad-f597d7680eaf")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c36d7f18-af6e-4f55-92e9-9a61132db797")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "8546acc7-2942-4086-93a6-92e029572140")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ad6da2e6-87eb-4dcc-8937-3ec055375474")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 1.04 0)
			(end 1.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "27cdb6ab-a16d-4c73-831e-0bd37fd8a1ef")
		)
		(fp_line
			(start 11.66 0)
			(end 10.97 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "219c98a6-28ca-44a0-85ad-8150b86badc5")
		)
		(fp_rect
			(start 1.73 -1.72)
			(end 10.97 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "cb1837ec-9f41-4b2b-a79c-32ce64c562fa")
		)
		(fp_rect
			(start -1.05 -1.85)
			(end 13.75 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "358de4d6-da4b-4b36-a481-89ffc187c83c")
		)
		(fp_line
			(start 0 0)
			(end 1.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b1b60eac-630c-4070-8b26-1685c4b0869d")
		)
		(fp_line
			(start 12.7 0)
			(end 10.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "869f5771-9101-487e-b640-875b671288d8")
		)
		(fp_rect
			(start 1.85 -1.6)
			(end 10.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "e5bcea7d-36fb-4f3c-bef4-f6e97c613948")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 0)
			(layer "F.Fab")
			(uuid "123153d6-37a0-4440-a82b-f1a9f9277a6b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO5")
			(pintype "passive")
			(uuid "a177b8f9-1844-4766-85b1-fce58f074eb3")
		)
		(pad "2" thru_hole circle
			(at 12.7 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-F)")
			(pintype "passive")
			(uuid "4882499f-3991-4a4e-8ea0-c6ec384ee216")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(uuid "2308fd8c-760d-4b34-afe0-7e8a48c4ed59")
		(at 35.0975 56.848333)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R7"
			(at 6.35 -2.72 0)
			(layer "F.SilkS")
			(uuid "5db3ce5f-3f93-40de-881b-f66650cf774a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100"
			(at 6.35 2.72 0)
			(layer "F.Fab")
			(uuid "1ce77d58-4beb-41a4-9d97-d32bda5afd14")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.koaglobal.com/-/media/Files/KOA_Global/EN/product/commonpdf/mos.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bbdf2531-7f66-4af3-b5e1-9cfd277eaf93")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9bd3eff5-23ec-459e-8165-cb7170b95c39")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7f633b38-c251-415a-8065-75f81e9b3d92")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f16d8856-d45a-46cd-8c29-093509db23d3")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 1.04 0)
			(end 1.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa054bc5-28bb-405c-a473-ec9f215b997c")
		)
		(fp_line
			(start 11.66 0)
			(end 10.97 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f009dd6d-305e-40cf-85da-6f4dbac1204f")
		)
		(fp_rect
			(start 1.73 -1.72)
			(end 10.97 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "a8f30bce-bc7e-4cb1-a7a8-57bd8cca945b")
		)
		(fp_rect
			(start -1.05 -1.85)
			(end 13.75 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "60ca56fa-2834-4933-a9fb-01d4dfb7104f")
		)
		(fp_line
			(start 0 0)
			(end 1.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f3e011d-e7fe-4552-82ec-68fb5453f711")
		)
		(fp_line
			(start 12.7 0)
			(end 10.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2958a12-25d3-4785-9373-e87d1677f52f")
		)
		(fp_rect
			(start 1.85 -1.6)
			(end 10.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "7c40899c-04b5-4286-96d8-3235b1284650")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 0)
			(layer "F.Fab")
			(uuid "4d52dba3-c427-4529-a13c-c69bdfd7a29b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO6")
			(pintype "passive")
			(uuid "0b09c759-a367-40d6-a715-49dc43370aa8")
		)
		(pad "2" thru_hole circle
			(at 12.7 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-G)")
			(pintype "passive")
			(uuid "0697d8e5-799e-44a2-a633-a783fd852c00")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(uuid "2f009aed-aac7-416f-9cf6-d0da51f7691c")
		(at 35.0975 61.674167)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R5"
			(at 6.35 -2.72 0)
			(layer "F.SilkS")
			(uuid "e39b77bc-64b3-41df-9336-defa0f512b15")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100"
			(at 6.35 2.72 0)
			(layer "F.Fab")
			(uuid "3bea2a4e-31cc-4145-a8ad-5112588acfea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.koaglobal.com/-/media/Files/KOA_Global/EN/product/commonpdf/mos.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e2222b37-0064-42ed-b7cb-c08c9e6a26a6")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e3409e1-4934-48de-b5d3-e3f03f728e19")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "cb4bd155-c045-4aa5-9fae-45d522937313")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6b696b1e-45b2-4a0c-8285-4bfa49fb9288")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 1.04 0)
			(end 1.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f357f350-4b8c-4fa9-aabe-35165efac669")
		)
		(fp_line
			(start 11.66 0)
			(end 10.97 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "34d1178e-dd87-4525-bb3e-274968c1f631")
		)
		(fp_rect
			(start 1.73 -1.72)
			(end 10.97 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "d94d5c83-bc9a-4add-86df-0c8b25080e4b")
		)
		(fp_rect
			(start -1.05 -1.85)
			(end 13.75 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "59d6d738-4880-440c-9318-7bb67659120c")
		)
		(fp_line
			(start 0 0)
			(end 1.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2abfa18e-8c61-4d50-a9fb-8972008d3bb2")
		)
		(fp_line
			(start 12.7 0)
			(end 10.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "40e946ea-2f2e-47f7-ac9f-2ef27f23338e")
		)
		(fp_rect
			(start 1.85 -1.6)
			(end 10.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "1d5118a4-4292-4d67-8d04-e195ed621bf6")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 0)
			(layer "F.Fab")
			(uuid "67d7b706-6ed3-4ea2-9559-cc01badba41f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO7")
			(pintype "passive")
			(uuid "bfd9ff82-da0c-48d9-a350-dbf1ac61df96")
		)
		(pad "2" thru_hole circle
			(at 12.7 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-E)")
			(pintype "passive")
			(uuid "abdd0f26-fea7-4f61-b92c-07ec77c96689")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_DIP_SPSTx01_Slide_9.78x4.72mm_W7.62mm_P2.54mm"
		(layer "F.Cu")
		(uuid "48bb0baa-70ec-4a02-89b2-238a5662a063")
		(at 120.2325 119.0125)
		(descr "1x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x4.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
		(tags "DIP Switch SPST Slide 7.62mm 300mil")
		(property "Reference" "REF**"
			(at 3.81 -3.42 0)
			(layer "F.SilkS")
			(uuid "e437f303-eaa4-49dc-821a-a4271e78c5a3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_DIP_SPSTx01_Slide_9.78x4.72mm_W7.62mm_P2.54mm"
			(at 3.81 3.42 0)
			(layer "F.Fab")
			(uuid "b9e6a8b9-1c64-4644-a887-0514d133a226")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "27ac4a0d-c6b8-4ce6-9554-b0d73efb9c89")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "51e01696-363b-4aac-becf-1a31c71e86db")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "button_switch/DIP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "4dc6100c-bb27-4bff-bd8f-e1bd0077c3a5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.38 -2.66)
			(end -1.38 -1.277)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1070366a-d472-494a-b73c-9694bccf86aa")
		)
		(fp_line
			(start -1.38 -2.66)
			(end 0.003 -2.66)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "61ceb147-334f-4103-a458-c814c53cdca1")
		)
		(fp_line
			(start -1.14 -2.42)
			(end -1.14 2.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8278b3d7-334c-4bf0-af0d-5f4e0d186825")
		)
		(fp_line
			(start -1.14 -2.42)
			(end 8.76 -2.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad9347d7-a846-4a50-acbe-3b0824199151")
		)
		(fp_line
			(start -1.14 2.42)
			(end 8.76 2.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48feb758-5915-4f39-896d-0db315bb597f")
		)
		(fp_line
			(start 3.133333 -0.635)
			(end 3.133333 0.635)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7858c84d-310c-4f53-87d1-0b90425bb910")
		)
		(fp_line
			(start 8.76 -2.42)
			(end 8.76 2.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "341406c5-8378-4e78-a7ec-5e6b7421ec71")
		)
		(fp_rect
			(start 1.78 -0.635)
			(end 3.133333 0.635)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "978f931d-f194-47dc-b94a-1c6963c4c3d8")
		)
		(fp_rect
			(start 1.78 -0.635)
			(end 5.84 0.635)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "c9924f7e-2ba4-4cfb-8899-1a8e23e0625a")
		)
		(fp_rect
			(start -1.33 -2.67)
			(end 8.95 2.67)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "ef87163e-4e0e-404d-b4ee-12450a098601")
		)
		(fp_line
			(start -1.08 -1.36)
			(end -0.08 -2.36)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a560e8a1-a96a-4267-899c-3f9c06fe240c")
		)
		(fp_line
			(start -1.08 2.36)
			(end -1.08 -1.36)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ddad8f41-80d2-4d76-b049-8e51e4c9558b")
		)
		(fp_line
			(start -0.08 -2.36)
			(end 8.7 -2.36)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f3489abf-540d-49f1-bf2d-5afaba54d5ef")
		)
		(fp_line
			(start 3.133333 -0.635)
			(end 3.133333 0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d0b64e0a-c910-499d-9d54-189fe9e8cec6")
		)
		(fp_line
			(start 8.7 -2.36)
			(end 8.7 2.36)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a7630db-1441-4dd4-ad1b-9abc63db4a01")
		)
		(fp_line
			(start 8.7 2.36)
			(end -1.08 2.36)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d0dd0ba5-b866-4f57-bf41-482ca8a6efd4")
		)
		(fp_rect
			(start 1.78 -0.635)
			(end 3.133333 0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "aa49b2c5-f97c-413a-8fca-6eb148d9cb0a")
		)
		(fp_rect
			(start 1.78 -0.635)
			(end 5.84 0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "800da15d-8666-46a0-8da9-7968cf22cda9")
		)
		(fp_text user "on"
			(at 5.365 -1.4975 0)
			(layer "F.Fab")
			(uuid "2e09a689-2186-4cdd-9a4f-a089f0f7a7b2")
			(effects
				(font
					(size 0.6 0.6)
					(thickness 0.09)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 7.27 0 90)
			(layer "F.Fab")
			(uuid "db53eb83-6803-49e2-b970-4a20af6b4bdd")
			(effects
				(font
					(size 0.6 0.6)
					(thickness 0.09)
				)
			)
		)
		(point
			(at 124.0425 119.0125)
			(size 1.27)
			(layer "F.Fab")
			(uuid "09582b73-2e04-44c0-9ea7-be69e7c26bab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(uuid "53e5ae53-b3a6-4b31-8ba4-345de29bfb55")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "e2f93b6f-d60f-4c43-a7bf-029d8cf102c3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx01_Slide_9.78x4.72mm_W7.62mm_P2.54mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Connector:External Attach for Slide"
		(layer "F.Cu")
		(uuid "48f0ce44-27c9-41c7-bf7d-bcce2d7e6fb4")
		(at 71.5 97)
		(descr "THT Pads for external objects")
		(tags "external, placeholder")
		(property "Reference" "SW4"
			(at 0 -2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "04455cf5-7ed7-48d7-8552-53154eebe662")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "SW_Slide_DPDT"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "7efadb3b-0c60-4eab-b2a0-c8523783b3dd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3e5e706f-07e5-403f-a87a-14ad42be2f77")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Slide Switch, dual pole double throw"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "646ab83e-f7fb-4dcf-888a-acaab4bf0dab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/57a6baab-f7c8-42b0-be47-aaed122e5046")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "6" "5" "4")
			)
		)
		(attr through_hole exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_rect
			(start -4 -1.5)
			(end 4 1.5)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "5fcbe659-334e-4c05-b362-415563d9e159")
		)
		(pad "3" thru_hole circle
			(at -2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-A)")
			(pinfunction "C_3")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(uuid "45a39db4-bab6-417f-ad27-949131a36bfb")
		)
		(pad "4" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "A_4")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(uuid "5e8a4f95-7f2e-4a79-8758-43f939de2530")
		)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T_NO_CK_PTS125Sx85PSMTR"
		(layer "F.Cu")
		(uuid "5bf3e674-9048-4e62-a98b-1ea065f4c86d")
		(at 124 106)
		(descr "Tactile switch, 12x12 mm, H8.5 mm, round actuator, with pegs, gullwing terminals, https://www.ckswitches.com/media/1462/pts125.pdf")
		(tags "button tactile switch SPST 1P1T C&K")
		(property "Reference" "REF**"
			(at 0 -7.3 0)
			(layer "F.SilkS")
			(uuid "7353eaa8-e33a-4569-9fd0-04f23d4dfcd8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push_1P1T_NO_CK_PTS125Sx85PSMTR"
			(at 0 7.1 0)
			(layer "F.Fab")
			(uuid "d5b998e0-d33b-47ea-be69-4e8742f31c33")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3bfac72b-5e16-4ab6-9ec5-d9ad693d4fa1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5eba0fde-9a2d-47d6-9ab1-60e2771155cc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -6.2 -4.6)
			(end -4.6 -6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b48e3575-ec96-48d5-8e7f-3832902a811e")
		)
		(fp_line
			(start -6.2 -3.45)
			(end -6.2 -4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "41355dc8-e565-4042-b01f-7752fd638399")
		)
		(fp_line
			(start -6.2 -1.55)
			(end -6.2 1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df0c988c-186f-4259-a0ca-e18dd0013aec")
		)
		(fp_line
			(start -6.2 3.45)
			(end -6.2 4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8db8c655-7d70-4b88-a07b-fe125e0830a4")
		)
		(fp_line
			(start -6.2 4.6)
			(end -4.6 6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b4f3265-42e5-4dce-b2f5-feaa74e8e29c")
		)
		(fp_line
			(start -4.6 -6.2)
			(end 4.6 -6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b70e2db8-20f3-47f0-984e-30718f01c7fe")
		)
		(fp_line
			(start -4.6 6.2)
			(end 4.6 6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b3cc5d7e-a4ea-4dfe-920e-d459d8465479")
		)
		(fp_line
			(start 4.6 -6.2)
			(end 6.2 -4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "52e0b7bf-01d7-4ed9-babe-c8a959868b99")
		)
		(fp_line
			(start 4.6 6.2)
			(end 6.2 4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30ef9cab-d2e4-4fda-b72a-fe84058f76d3")
		)
		(fp_line
			(start 6.2 -3.45)
			(end 6.2 -4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "69699ef8-7eba-4ae8-aba0-7240f0dab938")
		)
		(fp_line
			(start 6.2 -1.55)
			(end 6.2 1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64d0e68d-0898-4706-bb20-d196bdb5e143")
		)
		(fp_line
			(start 6.2 3.45)
			(end 6.2 4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb0d14ed-6206-4906-8cda-3021e5fde4af")
		)
		(fp_line
			(start -8.4 -6.25)
			(end 8.4 -6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6b28f7a-35c5-43a7-bd93-80bb9c119a92")
		)
		(fp_line
			(start -8.4 6.25)
			(end -8.4 -6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7359d477-bd6a-4ac7-a6ed-84cc59541758")
		)
		(fp_line
			(start 8.4 -6.25)
			(end 8.4 6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "015eaac0-f7f2-44df-bced-a3cb48ab4e8a")
		)
		(fp_line
			(start 8.4 6.25)
			(end -8.4 6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca3b5182-593e-4912-891a-75ea19f73667")
		)
		(fp_line
			(start -6 -4.5)
			(end -6 4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4f5743f8-8c7b-472d-986d-d3e11c97dca9")
		)
		(fp_line
			(start -6 -4.5)
			(end -4.5 -6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f72910a8-e518-405c-9f6d-3b69626cd915")
		)
		(fp_line
			(start -4.5 6)
			(end -6 4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f64ae13-0333-4203-bee9-ab50a8342efa")
		)
		(fp_line
			(start -4.5 6)
			(end 4.5 6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8dcac95e-5c33-4e33-b963-f7a8532ff7ae")
		)
		(fp_line
			(start 4.5 -6)
			(end -4.5 -6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f713583-0b84-4eed-aff2-5cd72e44aef7")
		)
		(fp_line
			(start 4.5 -6)
			(end 6 -4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7dad89be-b2a2-4ee4-885f-f02c4cbf470f")
		)
		(fp_line
			(start 6 4.5)
			(end 4.5 6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f823d9e7-4a18-4efb-a2bf-a98781a98db1")
		)
		(fp_line
			(start 6 4.5)
			(end 6 -4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f054aef-a20c-4779-8883-bdc5fbfcc966")
		)
		(fp_circle
			(center 0 0)
			(end 3.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "11c81ec1-c376-4458-984c-5d8c935aa275")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "648ba50e-20e7-46b8-bb2b-9efbda4f03d7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 -4.5)
			(size 2 2)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(uuid "a945ccd3-7cb4-452f-8684-9141e8ce73a1")
		)
		(pad "" np_thru_hole circle
			(at 0 4.5)
			(size 2 2)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(uuid "8d38cef6-8b5e-4911-b654-7337c55f31c9")
		)
		(pad "1" smd roundrect
			(at -7.15 -2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "7d033c98-e10f-4a77-8324-aff18fab71a4")
		)
		(pad "1" smd roundrect
			(at 7.15 -2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "b5dcf31b-e2bb-4797-bc50-d5536e04d335")
		)
		(pad "2" smd roundrect
			(at -7.15 2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "e10853e4-97ab-4080-9c19-be9248702dea")
		)
		(pad "2" smd roundrect
			(at 7.15 2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "76769f50-81e7-4b4a-9613-28a3afb442e2")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_CK_PTS125Sx85PSMTR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector:External Attach for Push Button"
		(layer "F.Cu")
		(uuid "67a4f419-f7ec-4b74-8de7-dd779609f2fd")
		(at 47.8375 100.5)
		(descr "THT Pads for external push button")
		(tags "external, button, placeholder")
		(property "Reference" "SW2"
			(at 0 -2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "ef274aa5-39e7-4866-8b82-2aa0eef4f39f")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "SW_Push"
			(at 0 2 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "23169a44-77be-4f62-81ff-41555f8cde73")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8ca7e054-0940-42aa-a414-3a18b4c7dfcb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "24225b43-c7bf-4c15-8813-49cb2fa69d3f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/4509c1c3-31c5-4283-83c4-70c8f2d30f71")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_rect
			(start -4 -1.5)
			(end 4 1.5)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "5cca1ded-e7a0-4c43-9e6c-1e861266b59e")
		)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(A1-GPIO17)")
			(pinfunction "1_1")
			(pintype "passive")
			(uuid "bec48ebb-8e84-498d-8ee3-4538da61a5ae")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "2_2")
			(pintype "passive")
			(uuid "92d8e1b2-1c8d-4d6b-b08a-f8ca4304ba52")
		)
		(embedded_fonts no)
	)
	(footprint "Module:RaspberryPi_Pico_Common_THT"
		(layer "F.Cu")
		(uuid "77d25365-aa54-4de3-a592-adfaa2eda288")
		(at 80.8175 74 -90)
		(descr "Raspberry Pi Pico common (Pico & Pico W) through-hole footprint, supports Raspberry Pi Pico 2, default socketed model has height of 8.51mm, https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf")
		(tags "module usb pcb antenna")
		(property "Reference" "A1"
			(at 20.6375 48.895 270)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "4a4c0211-fd69-44d6-b63b-e6a6cbded556")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify left)
			)
		)
		(property "Value" "RaspberryPi_Pico_W"
			(at 8.89 52.07 270)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "9a3d3a06-4857-4bf9-a222-c6bb5f39cbff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 8.89 24.13 270)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac473fa3-cfb3-4705-b334-c0829f933148")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Versatile and inexpensive wireless microcontroller module powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash, Infineon CYW43439 2.4GHz 802.11n wireless LAN; also supports Raspberry Pi Pico 2 W"
			(at 8.89 24.13 270)
			(layer "F.Fab")
			(hide yes)
			(uuid "da13d6ec-8d2b-4a23-ba2c-c9d486a85aee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "RaspberryPi?Pico?Common* RaspberryPi?Pico?W?SMD*")
		(path "/b879fa2d-0f67-4368-8d97-e6458f9ab5b6")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "30" "37" "1" "2" "4" "5" "6" "7" "9" "10" "11" "12" "14" "15"
					"16" "17" "19" "20" "39" "40" "3" "23" "28" "18" "13" "38" "8" "36"
					"21" "22" "24" "25" "26" "27" "29" "35" "31" "32" "34" "33"
				)
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.11 49.74)
			(end 2.727939 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "46a463d7-b6ee-4fab-9047-a87f21ed0883")
		)
		(fp_line
			(start 5.29 49.74)
			(end 3.652061 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8461f0b9-08b5-4a5e-90ca-11d6bde280e0")
		)
		(fp_line
			(start 12.49 49.74)
			(end 5.29 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ffe5611-f291-4daa-88c8-0549d5bcc291")
		)
		(fp_line
			(start 14.127939 49.74)
			(end 12.49 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d67059e-2efc-49e7-8a0c-36b92bfcf0e6")
		)
		(fp_line
			(start 15.052061 49.74)
			(end 18.89 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b295bdf-948b-4bcd-bcf0-e24005696086")
		)
		(fp_line
			(start 19.16 49.677)
			(end 19.16 -1.417)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eece7ed3-2591-4e4d-a9fd-76250996b03c")
		)
		(fp_line
			(start 1.38 48.82648)
			(end 1.38 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6b8ca7b-3624-4d7c-9486-ffeee4caf2db")
		)
		(fp_line
			(start 16.4 48.82648)
			(end 16.4 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6e68b374-bd76-451c-bdc9-165e41c175ab")
		)
		(fp_line
			(start 12.79 3.04)
			(end 4.99 3.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c3c5e62-ef9e-4d2d-a3d9-74e2c3d77a09")
		)
		(fp_line
			(start 1.38 1.82648)
			(end 1.38 46.43352)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "600165b7-2df0-49c8-9c6e-f59c6e704890")
		)
		(fp_line
			(start 16.4 1.82648)
			(end 16.4 46.43352)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f43a3c8b-d186-4f8c-b9a2-d00490f2faa6")
		)
		(fp_line
			(start 4.99 1.824)
			(end 4.99 3.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64069aa4-96e6-474b-97b9-45102ccb8b3b")
		)
		(fp_line
			(start 12.79 1.824)
			(end 12.79 3.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ab08ec92-f691-4f27-a5c6-102bc84521e5")
		)
		(fp_line
			(start -2.04 0.8)
			(end -2.04 -0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "291e82b6-edd1-4848-8fc7-07dae5654d8b")
		)
		(fp_line
			(start -1.72 -0.87)
			(end -1.72 49.13)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee203052-ec08-49db-a34f-c91e49b16dc9")
		)
		(fp_line
			(start 19.5 -0.87)
			(end 19.5 49.13)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "556583b1-9855-4d2d-8236-2f9405c631d5")
		)
		(fp_line
			(start -1.38 -1.417)
			(end -1.38 49.677)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "40e6b921-e3ab-48d4-bf16-7d82609220a3")
		)
		(fp_line
			(start -1.11 -1.48)
			(end 1.38 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3cb34300-fb64-4402-ab1a-f5eaa0156e56")
		)
		(fp_line
			(start 1.38 -1.48)
			(end 1.38 -0.56648)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b04b7ae-0d8b-4a93-8835-dc9776920c3d")
		)
		(fp_line
			(start 1.38 -1.48)
			(end 2.72794 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c9dd665f-72a7-40a2-a0f3-b40fbd739005")
		)
		(fp_line
			(start 3.652061 -1.48)
			(end 4.655 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bee7c4ad-fbf9-47dd-a20a-3a34103edc9e")
		)
		(fp_line
			(start 4.655 -1.48)
			(end 13.125 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60c21dee-73cb-453d-a423-5c228fbee416")
		)
		(fp_line
			(start 13.125 -1.48)
			(end 14.127939 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14094796-77e4-4202-a053-33a51102759d")
		)
		(fp_line
			(start 15.052061 -1.48)
			(end 16.4 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68e51eee-7877-46b0-9aca-5aaab682a981")
		)
		(fp_line
			(start 16.4 -1.48)
			(end 16.4 -0.56648)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "108d53be-e43d-43c6-b9ef-ca21f16a870e")
		)
		(fp_line
			(start 18.89 -1.48)
			(end 16.4 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ad4a479-9c4d-4be2-be4e-7378133080d8")
		)
		(fp_line
			(start 4.78 -1.96)
			(end 4.99 -1.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "035fbd3b-ad19-4bc6-8b2d-58dacd0442cd")
		)
		(fp_line
			(start 4.99 -1.96)
			(end 4.99 -0.564)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac4677de-7319-4c3d-bf33-9ddebfad8561")
		)
		(fp_line
			(start 12.79 -1.96)
			(end 12.79 -0.564)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c85d827-6992-4f74-bc7a-e92cb7085d86")
		)
		(fp_line
			(start 13 -1.96)
			(end 12.79 -1.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e799a3f-6ccc-4bc3-8c76-53603589ef56")
		)
		(fp_line
			(start 4.78 -2.78)
			(end 4.78 -1.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86214e53-de7f-4a82-919d-8b72e0e01fa4")
		)
		(fp_line
			(start 4.78 -2.78)
			(end 13 -2.78)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8159f0f-6f00-406c-9043-8f59299f12c2")
		)
		(fp_line
			(start 13 -2.78)
			(end 13 -1.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed0f85a5-f291-425a-8842-af82ab27a81f")
		)
		(fp_arc
			(start -1.11 49.74)
			(mid -1.541364 49.561364)
			(end -1.72 49.13)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ffcd6ef1-2dc0-48c7-a0d0-c116699136db")
		)
		(fp_arc
			(start 19.5 49.13)
			(mid 19.321335 49.561335)
			(end 18.89 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a24bc75-a0e5-4785-9db4-f6af43e64c44")
		)
		(fp_arc
			(start -1.72 -0.87)
			(mid -1.541335 -1.301335)
			(end -1.11 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ad10628-31a5-48e6-92f9-061498973d90")
		)
		(fp_arc
			(start 18.89 -1.48)
			(mid 19.321335 -1.301335)
			(end 19.5 -0.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2cb023cf-0053-41d5-b3fc-9d749269e737")
		)
		(fp_circle
			(center 3.19 47.63)
			(end 4.24 47.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "Dwgs.User")
			(uuid "48e591d3-a339-41b3-95f9-a01795cbf7bb")
		)
		(fp_circle
			(center 14.59 47.63)
			(end 15.64 47.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "Dwgs.User")
			(uuid "51a02694-cf1e-401e-9b6c-a9fd70f3f77d")
		)
		(fp_circle
			(center 3.19 0.63)
			(end 4.24 0.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "Dwgs.User")
			(uuid "c37f7025-4e98-40ed-8b39-d6ea92eb206e")
		)
		(fp_circle
			(center 14.59 0.63)
			(end 15.64 0.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "Dwgs.User")
			(uuid "673ba770-e513-4aff-bf19-95a346a49a48")
		)
		(fp_poly
			(pts
				(xy 4.39 -3.17) (xy 13.39 -3.17) (xy 13.39 -1.62) (xy 20.43 -1.62) (xy 20.43 50.68) (xy -2.65 50.68)
				(xy -2.65 -1.62) (xy 4.39 -1.62)
			)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "0d1c3db1-1677-47d9-8fcc-18d749a8e79c")
		)
		(fp_line
			(start 18.89 49.63)
			(end -1.11 49.63)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a1507cf8-101b-415c-8764-9b82fb6cc358")
		)
		(fp_line
			(start -1.61 49.13)
			(end -1.61 -0.37)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb3e9353-8517-4055-86b0-88711ffc93f5")
		)
		(fp_line
			(start 4.265 10.055)
			(end 4.265 11.205)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f79f1d9-b918-4e18-8b34-2c2c391045fa")
		)
		(fp_line
			(start 6.515 10.055)
			(end 6.515 11.205)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "727db3c1-2150-4777-a226-3344e01c1f6f")
		)
		(fp_line
			(start -1.61 -0.37)
			(end -0.61 -1.37)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dea77f85-842b-45f6-9195-4693694d00b7")
		)
		(fp_line
			(start 19.39 -0.87)
			(end 19.39 49.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e53a9e0-f548-457e-95f6-15ab3ffa200f")
		)
		(fp_line
			(start -0.61 -1.37)
			(end 18.89 -1.37)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d139e30-821e-4dba-bdd2-0d0e54b998f3")
		)
		(fp_rect
			(start 3.79 8.505)
			(end 6.99 12.755)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "1fc35dff-8f5b-4898-8d90-07e8017dc1b7")
		)
		(fp_rect
			(start 2.39 3.03)
			(end 3.99 3.83)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "ba4134de-bab1-46d5-80bb-9e745e1d31db")
		)
		(fp_rect
			(start 2.69 3.03)
			(end 3.69 3.83)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "4cb46abf-b15d-4bf8-a6b4-d642e0568417")
		)
		(fp_arc
			(start -1.11 49.63)
			(mid -1.463553 49.483553)
			(end -1.61 49.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9fad9bd-9983-41a4-8206-f2decec2e67e")
		)
		(fp_arc
			(start 19.39 49.13)
			(mid 19.243553 49.483553)
			(end 18.89 49.63)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c89bbae4-e876-4e84-bfe9-14d9deb69490")
		)
		(fp_arc
			(start 6.515 11.205)
			(mid 5.39 12.33)
			(end 4.265 11.205)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ff9b566-4647-46cf-96d1-028b11269914")
		)
		(fp_arc
			(start 4.265 10.055)
			(mid 5.39 8.93)
			(end 6.515 10.055)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c4f2d77-82f1-48ae-aded-5a374283714a")
		)
		(fp_arc
			(start 18.89 -1.37)
			(mid 19.243553 -1.223553)
			(end 19.39 -0.87)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31cae337-67a0-48da-87d7-48f2b1778508")
		)
		(fp_poly
			(pts
				(xy 12.68 2.93) (xy 12.68 -2.07) (xy 12.89 -2.07) (xy 12.89 -2.67) (xy 4.89 -2.67) (xy 4.89 -2.07)
				(xy 5.1 -2.07) (xy 5.1 2.93)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "0f18e3d6-0acc-4de0-8004-939f1a3ccb79")
		)
		(fp_text user "Keep Out"
			(at 8.89 45.72 270)
			(unlocked yes)
			(layer "Cmts.User")
			(uuid "013376cb-92f1-47f7-872f-907b69675c6b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "Possible Antenna"
			(at 8.89 43.815 270)
			(unlocked yes)
			(layer "Cmts.User")
			(uuid "08a8964c-2476-4aae-936d-9559e9a0f9d8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "USB Cable"
			(at 8.89 -13.335 270)
			(unlocked yes)
			(layer "Cmts.User")
			(uuid "2d8acffe-6a1f-48b5-b1d8-ed15d464664e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 8.89 24.13 0)
			(layer "F.Fab")
			(uuid "7f08a5cf-2763-42f5-8bb8-ab5ed6c5d133")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net "/GPIO0")
			(pinfunction "GPIO0_1")
			(pintype "bidirectional")
			(uuid "87386b28-7d40-48ee-95e0-a79d0472984b")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO1")
			(pinfunction "GPIO1_2")
			(pintype "bidirectional")
			(uuid "acba2426-534c-40c8-8cc1-304e8f4b9576")
		)
		(pad "3" thru_hole custom
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_3")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "f70e2e97-a1d3-4007-891d-26a1214a6185")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO2")
			(pinfunction "GPIO2_4")
			(pintype "bidirectional")
			(uuid "f9750b0b-b217-44d8-a1f3-c7e5d78a5c47")
		)
		(pad "5" thru_hole circle
			(at 0 10.16 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO3")
			(pinfunction "GPIO3_5")
			(pintype "bidirectional")
			(uuid "8fd91f9a-d265-4705-8b27-06428ef50202")
		)
		(pad "6" thru_hole circle
			(at 0 12.7 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO4")
			(pinfunction "GPIO4_6")
			(pintype "bidirectional")
			(uuid "99f4855d-945f-49ef-be54-72d99533740f")
		)
		(pad "7" thru_hole circle
			(at 0 15.24 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO5")
			(pinfunction "GPIO5_7")
			(pintype "bidirectional")
			(uuid "a99814e8-afad-47e3-a777-102fbfa4b294")
		)
		(pad "8" thru_hole custom
			(at 0 17.78 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_8")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "7dd8760d-6467-4524-81eb-0abdece9fb1d")
		)
		(pad "9" thru_hole circle
			(at 0 20.32 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO6")
			(pinfunction "GPIO6_9")
			(pintype "bidirectional")
			(uuid "2c51de86-cc3f-4900-bab4-5c400463ca6b")
		)
		(pad "10" thru_hole circle
			(at 0 22.86 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO7")
			(pinfunction "GPIO7_10")
			(pintype "bidirectional")
			(uuid "7f9f3e20-f777-4529-98c4-a0588e5663d1")
		)
		(pad "11" thru_hole circle
			(at 0 25.4 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO8")
			(pinfunction "GPIO8_11")
			(pintype "bidirectional")
			(uuid "3278b79d-148c-4b65-bca5-ceca64e04fa6")
		)
		(pad "12" thru_hole circle
			(at 0 27.94 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO9")
			(pinfunction "GPIO9_12")
			(pintype "bidirectional")
			(uuid "624e2f73-9654-4c6f-98db-8960010ff55d")
		)
		(pad "13" thru_hole custom
			(at 0 30.48 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_13")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "a60605f1-f8ff-41c6-a9f3-73e36b49f82b")
		)
		(pad "14" thru_hole circle
			(at 0 33.02 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO10-Pad14)")
			(pinfunction "GPIO10_14")
			(pintype "bidirectional+no_connect")
			(uuid "abcdf859-4b98-4b8b-a8f6-9cf15c6f919b")
		)
		(pad "15" thru_hole circle
			(at 0 35.56 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO11-Pad15)")
			(pinfunction "GPIO11_15")
			(pintype "bidirectional+no_connect")
			(uuid "a574a151-a13f-4d26-b5bb-9235dc63921a")
		)
		(pad "16" thru_hole circle
			(at 0 38.1 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO12-Pad16)")
			(pinfunction "GPIO12_16")
			(pintype "bidirectional+no_connect")
			(uuid "de3f1615-dc50-4dc2-ae2c-e155e0826336")
		)
		(pad "17" thru_hole circle
			(at 0 40.64 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO13-Pad17)")
			(pinfunction "GPIO13_17")
			(pintype "bidirectional+no_connect")
			(uuid "9e161f2b-dfd6-41d9-9fcc-2787a3da58a4")
		)
		(pad "18" thru_hole custom
			(at 0 43.18 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_18")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "72f0e6af-fab5-4beb-8fe1-72d1b0f75173")
		)
		(pad "19" thru_hole circle
			(at 0 45.72 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO14-Pad19)")
			(pinfunction "GPIO14_19")
			(pintype "bidirectional+no_connect")
			(uuid "3946ff01-8378-4321-8394-a0c578792947")
		)
		(pad "20" thru_hole circle
			(at 0 48.26 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO15-Pad20)")
			(pinfunction "GPIO15_20")
			(pintype "bidirectional+no_connect")
			(uuid "ed698d27-d460-4072-882d-c94ca1624bfd")
		)
		(pad "21" thru_hole circle
			(at 17.78 48.26 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(A1-GPIO16)")
			(pinfunction "GPIO16_21")
			(pintype "bidirectional")
			(uuid "a118f352-d43d-4633-b3ea-30c4548bd4d3")
		)
		(pad "22" thru_hole circle
			(at 17.78 45.72 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(A1-GPIO17)")
			(pinfunction "GPIO17_22")
			(pintype "bidirectional")
			(uuid "2b12cd53-c561-4432-a8e8-3af3731d7799")
		)
		(pad "23" thru_hole custom
			(at 17.78 43.18 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_23")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "1c5dfb89-8f99-47ff-b498-65f403f07513")
		)
		(pad "24" thru_hole circle
			(at 17.78 40.64 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(A1-GPIO18)")
			(pinfunction "GPIO18_24")
			(pintype "bidirectional")
			(uuid "3eaf4d58-6f0d-41dc-9523-9873d926097d")
		)
		(pad "25" thru_hole circle
			(at 17.78 38.1 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO19-Pad25)")
			(pinfunction "GPIO19_25")
			(pintype "bidirectional+no_connect")
			(uuid "9ae0a38b-6546-4972-b977-1e92fb96b821")
		)
		(pad "26" thru_hole circle
			(at 17.78 35.56 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO20-Pad26)")
			(pinfunction "GPIO20_26")
			(pintype "bidirectional+no_connect")
			(uuid "dcd409d3-1317-45c7-9492-df8e377654ae")
		)
		(pad "27" thru_hole circle
			(at 17.78 33.02 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO21-Pad27)")
			(pinfunction "GPIO21_27")
			(pintype "bidirectional+no_connect")
			(uuid "afdc25a9-657a-4a83-9068-c797fc5d5c3e")
		)
		(pad "28" thru_hole custom
			(at 17.78 30.48 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_28")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "616d0145-0d07-4406-8636-ab9eb891f112")
		)
		(pad "29" thru_hole circle
			(at 17.78 27.94 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO22-Pad29)")
			(pinfunction "GPIO22_29")
			(pintype "bidirectional+no_connect")
			(uuid "105a6d6a-e18e-4e0c-aa92-8b5792c3b0c4")
		)
		(pad "30" thru_hole circle
			(at 17.78 25.4 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-RUN-Pad30)")
			(pinfunction "RUN_30")
			(pintype "passive+no_connect")
			(uuid "e7bda639-027e-4cd7-971b-8beb4a7ddb34")
		)
		(pad "31" thru_hole circle
			(at 17.78 22.86 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO26_ADC0-Pad31)")
			(pinfunction "GPIO26_ADC0_31")
			(pintype "bidirectional+no_connect")
			(uuid "1a840cbc-ee21-413f-9161-462cedba092b")
		)
		(pad "32" thru_hole circle
			(at 17.78 20.32 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO27_ADC1-Pad32)")
			(pinfunction "GPIO27_ADC1_32")
			(pintype "bidirectional+no_connect")
			(uuid "67808a64-c00e-4d33-87c8-30d87d209917")
		)
		(pad "33" thru_hole custom
			(at 17.78 17.78 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-AGND-Pad33)")
			(pinfunction "AGND_33")
			(pintype "power_out+no_connect")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "1268e3ff-9ed8-4120-b2d6-e6d1e46c4ef5")
		)
		(pad "34" thru_hole circle
			(at 17.78 15.24 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-GPIO28_ADC2-Pad34)")
			(pinfunction "GPIO28_ADC2_34")
			(pintype "bidirectional+no_connect")
			(uuid "087faf46-4ac1-45f7-bba0-ee4e83941df7")
		)
		(pad "35" thru_hole circle
			(at 17.78 12.7 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF_35")
			(pintype "power_in+no_connect")
			(uuid "701e2a9d-3494-4c25-9852-130ddd810f65")
		)
		(pad "36" thru_hole circle
			(at 17.78 10.16 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-3V3-Pad36)")
			(pinfunction "3V3_36")
			(pintype "power_out+no_connect")
			(uuid "da7fffd9-45eb-4227-a405-59f39df94371")
		)
		(pad "37" thru_hole circle
			(at 17.78 7.62 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-3V3_EN-Pad37)")
			(pinfunction "3V3_EN_37")
			(pintype "passive+no_connect")
			(uuid "ad7bacf2-4489-4e3e-af6a-6fbe4f952f3a")
		)
		(pad "38" thru_hole custom
			(at 17.78 5.08 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_38")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "90ec4130-28bd-439b-8ad6-1ea8054176f5")
		)
		(pad "39" thru_hole circle
			(at 17.78 2.54 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(A1-VSYS)")
			(pinfunction "VSYS_39")
			(pintype "power_in")
			(uuid "6fd36d5f-ea72-474a-8cbc-cb8c18550f8f")
		)
		(pad "40" thru_hole circle
			(at 17.78 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(A1-VBUS-Pad40)")
			(pinfunction "VBUS_40")
			(pintype "power_out+no_connect")
			(uuid "df8ef5a5-f817-46e0-8b46-0efc34ce3d29")
		)
		(zone
			(layers "F.Cu" "B.Cu" "F.Paste" "B.Paste")
			(uuid "9d4097c6-68d1-44fb-88b2-83a0f6ded449")
			(name "Antenna Copper Keep Out")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 31.697605 80.49) (xy 35.347605 75.79) (xy 39.6875 75.79) (xy 39.6875 89.99) (xy 35.347605 89.99)
					(xy 31.697605 85.29) (xy 30.6875 85.29) (xy 30.6875 80.49)
				)
			)
		)
		(zone
			(layer "F.CrtYd")
			(uuid "ecb540ee-f291-4f8a-959b-acb58a861e77")
			(name "USB Cable")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 84.3875 77.14) (xy 84.3875 78.95) (xy 83.9875 78.95) (xy 83.9875 86.83) (xy 84.3875 86.83)
					(xy 84.3875 88.64) (xy 103.8875 88.64) (xy 103.8875 77.14)
				)
			)
		)
		(group ""
			(uuid "a10bd319-2abd-4185-95c5-8774687fdfbb")
			(members "087faf46-4ac1-45f7-bba0-ee4e83941df7" "105a6d6a-e18e-4e0c-aa92-8b5792c3b0c4"
				"108d53be-e43d-43c6-b9ef-ca21f16a870e" "1268e3ff-9ed8-4120-b2d6-e6d1e46c4ef5"
				"1a840cbc-ee21-413f-9161-462cedba092b" "1c5dfb89-8f99-47ff-b498-65f403f07513"
				"2b04b7ae-0d8b-4a93-8835-dc9776920c3d" "2b12cd53-c561-4432-a8e8-3af3731d7799"
				"2c51de86-cc3f-4900-bab4-5c400463ca6b" "3278b79d-148c-4b65-bca5-ceca64e04fa6"
				"3946ff01-8378-4321-8394-a0c578792947" "3cb34300-fb64-4402-ab1a-f5eaa0156e56"
				"3eaf4d58-6f0d-41dc-9523-9873d926097d" "600165b7-2df0-49c8-9c6e-f59c6e704890"
				"616d0145-0d07-4406-8636-ab9eb891f112" "624e2f73-9654-4c6f-98db-8960010ff55d"
				"67808a64-c00e-4d33-87c8-30d87d209917" "6e68b374-bd76-451c-bdc9-165e41c175ab"
				"6fd36d5f-ea72-474a-8cbc-cb8c18550f8f" "701e2a9d-3494-4c25-9852-130ddd810f65"
				"72f0e6af-fab5-4beb-8fe1-72d1b0f75173" "7dd8760d-6467-4524-81eb-0abdece9fb1d"
				"7f9f3e20-f777-4529-98c4-a0588e5663d1" "87386b28-7d40-48ee-95e0-a79d0472984b"
				"8fd91f9a-d265-4705-8b27-06428ef50202" "90ec4130-28bd-439b-8ad6-1ea8054176f5"
				"99f4855d-945f-49ef-be54-72d99533740f" "9ad4a479-9c4d-4be2-be4e-7378133080d8"
				"9ae0a38b-6546-4972-b977-1e92fb96b821" "9e161f2b-dfd6-41d9-9fcc-2787a3da58a4"
				"a118f352-d43d-4633-b3ea-30c4548bd4d3" "a574a151-a13f-4d26-b5bb-9235dc63921a"
				"a60605f1-f8ff-41c6-a9f3-73e36b49f82b" "a99814e8-afad-47e3-a777-102fbfa4b294"
				"abcdf859-4b98-4b8b-a8f6-9cf15c6f919b" "acba2426-534c-40c8-8cc1-304e8f4b9576"
				"ad7bacf2-4489-4e3e-af6a-6fbe4f952f3a" "afdc25a9-657a-4a83-9068-c797fc5d5c3e"
				"c6b8ca7b-3624-4d7c-9486-ffeee4caf2db" "da7fffd9-45eb-4227-a405-59f39df94371"
				"dcd409d3-1317-45c7-9492-df8e377654ae" "de3f1615-dc50-4dc2-ae2c-e155e0826336"
				"df8ef5a5-f817-46e0-8b46-0efc34ce3d29" "e7bda639-027e-4cd7-971b-8beb4a7ddb34"
				"ed698d27-d460-4072-882d-c94ca1624bfd" "f43a3c8b-d186-4f8c-b9a2-d00490f2faa6"
				"f70e2e97-a1d3-4007-891d-26a1214a6185" "f9750b0b-b217-44d8-a1f3-c7e5d78a5c47"
			)
		)
		(group ""
			(uuid "18f7cbfd-90fd-4a35-a942-83989a13208b")
			(members "013376cb-92f1-47f7-872f-907b69675c6b" "08a8964c-2476-4aae-936d-9559e9a0f9d8"
				"2a24bc75-a0e5-4785-9db4-f6af43e64c44" "4ffe5611-f291-4daa-88c8-0549d5bcc291"
				"9d4097c6-68d1-44fb-88b2-83a0f6ded449" "ffcd6ef1-2dc0-48c7-a0d0-c116699136db"
			)
		)
		(group ""
			(uuid "f3893067-7c0c-4d53-a59f-a7864795ef46")
			(members "291e82b6-edd1-4848-8fc7-07dae5654d8b" "2cb023cf-0053-41d5-b3fc-9d749269e737"
				"40e6b921-e3ab-48d4-bf16-7d82609220a3" "4ad10628-31a5-48e6-92f9-061498973d90"
				"556583b1-9855-4d2d-8236-2f9405c631d5" "ee203052-ec08-49db-a34f-c91e49b16dc9"
				"eece7ed3-2591-4e4d-a9fd-76250996b03c"
			)
		)
		(group ""
			(uuid "fbfa79a6-c00e-43c7-9115-64511794da09")
			(members "035fbd3b-ad19-4bc6-8b2d-58dacd0442cd" "1c3c5e62-ef9e-4d2d-a3d9-74e2c3d77a09"
				"3c85d827-6992-4f74-bc7a-e92cb7085d86" "3e799a3f-6ccc-4bc3-8c76-53603589ef56"
				"60c21dee-73cb-453d-a423-5c228fbee416" "64069aa4-96e6-474b-97b9-45102ccb8b3b"
				"86214e53-de7f-4a82-919d-8b72e0e01fa4" "ab08ec92-f691-4f27-a5c6-102bc84521e5"
				"ac4677de-7319-4c3d-bf33-9ddebfad8561" "ed0f85a5-f291-425a-8842-af82ab27a81f"
				"f8159f0f-6f00-406c-9043-8f59299f12c2"
			)
		)
		(group ""
			(uuid "27a714b9-4e1e-449c-8389-2e3f0c45c37e")
			(members "14094796-77e4-4202-a053-33a51102759d" "3d67059e-2efc-49e7-8a0c-36b92bfcf0e6"
				"46a463d7-b6ee-4fab-9047-a87f21ed0883" "48e591d3-a339-41b3-95f9-a01795cbf7bb"
				"51a02694-cf1e-401e-9b6c-a9fd70f3f77d" "673ba770-e513-4aff-bf19-95a346a49a48"
				"68e51eee-7877-46b0-9aca-5aaab682a981" "7b295bdf-948b-4bcd-bcf0-e24005696086"
				"8461f0b9-08b5-4a5e-90ca-11d6bde280e0" "bee7c4ad-fbf9-47dd-a20a-3a34103edc9e"
				"c37f7025-4e98-40ed-8b39-d6ea92eb206e" "c9dd665f-72a7-40a2-a0f3-b40fbd739005"
			)
		)
		(group ""
			(uuid "27ca16fa-57b4-4d13-b768-7c1652f6c6f4")
			(members "0d1c3db1-1677-47d9-8fcc-18d749a8e79c" "0f18e3d6-0acc-4de0-8004-939f1a3ccb79"
				"1fc35dff-8f5b-4898-8d90-07e8017dc1b7" "2d8acffe-6a1f-48b5-b1d8-ed15d464664e"
				"31cae337-67a0-48da-87d7-48f2b1778508" "3d139e30-821e-4dba-bdd2-0d0e54b998f3"
				"4cb46abf-b15d-4bf8-a6b4-d642e0568417" "5c4f2d77-82f1-48ae-aded-5a374283714a"
				"6e53a9e0-f548-457e-95f6-15ab3ffa200f" "6ff9b566-4647-46cf-96d1-028b11269914"
				"727db3c1-2150-4777-a226-3344e01c1f6f" "7f08a5cf-2763-42f5-8bb8-ab5ed6c5d133"
				"7f79f1d9-b918-4e18-8b34-2c2c391045fa" "a1507cf8-101b-415c-8764-9b82fb6cc358"
				"ba4134de-bab1-46d5-80bb-9e745e1d31db" "c89bbae4-e876-4e84-bfe9-14d9deb69490"
				"c9fad9bd-9983-41a4-8206-f2decec2e67e" "cb3e9353-8517-4055-86b0-88711ffc93f5"
				"dea77f85-842b-45f6-9195-4693694d00b7" "ecb540ee-f291-4f8a-959b-acb58a861e77"
			)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_PinSockets_H8.50mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD10_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_AddedHeaders_H2.54mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD10_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_H.step"
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD10_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W_AddedHeaders_H2.54mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD10_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_WH.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector:External Attach for Power"
		(layer "F.Cu")
		(uuid "782ee3eb-23f0-4689-aec4-53ef8e85ffe7")
		(at 71.5 103 180)
		(descr "THT Pads for external power delivery")
		(tags "external, power, battery")
		(property "Reference" "BT1"
			(at 0 -2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "96deba5a-82db-4a27-a37f-d27d46d756ab")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "3.3V"
			(at 0 2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "56bc90eb-6739-4413-8ccc-07a5058ab7d2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c3c51c6-3c7e-433d-b158-003c70b83e1d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Multiple-cell battery"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f53d583d-4924-4d6a-ac12-554833fe82ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d5141d59-fc5f-410c-93a7-6fcfff8982ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "DC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3b3d867e-79ce-45f5-a673-47814a04f8b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "91053008-61dc-46d8-918d-7dec4b0a469d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/536ee4f0-1a45-4a7f-b163-43de17281041")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_rect
			(start -4 -1.5)
			(end 4 1.5)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "b571192d-102e-460f-889b-858c3c918d89")
		)
		(pad "1" thru_hole circle
			(at -2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(A1-VSYS)")
			(pinfunction "+_1")
			(pintype "passive")
			(uuid "efe26fa6-4045-4096-bb4b-db562be49c6e")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(BT1--)")
			(pinfunction "-_2")
			(pintype "passive")
			(uuid "78463fc7-5773-48a4-a4ab-a572406ae6b5")
		)
		(embedded_fonts no)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "7c94d0f0-920d-4b7d-8a8c-4d04b5244f8e")
		(at 56.19 97)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, length*diameter=5.2*2.7mm^2, https://www.diodes.com/assets/Package-Files/DO-41-Plastic.pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D1"
			(at 3.81 -2.47 0)
			(layer "F.SilkS")
			(uuid "70ff41db-f51e-4c13-b145-8eaba585cb36")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "D_Schottky"
			(at 4 2.47 0)
			(layer "F.Fab")
			(uuid "a654744e-c69c-43bc-954f-5b508029ad97")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.farnell.com/datasheets/2308559.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8385169e-7cc2-4c5b-b538-d9d6b90012f1")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Schottky diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c75f011-0232-437f-a7df-754bea9d30b7")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "diode/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "48066677-2452-409a-aa0e-f71e7e9d5023")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/1cafdd5a-8dbf-4ccb-bd03-9d1d37cc1c1c")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 1.09 -1.47)
			(end 6.53 -1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfa1fdeb-41c5-41c4-84fa-b621f3e425aa")
		)
		(fp_line
			(start 1.09 -1.34)
			(end 1.09 -1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c26709af-b6aa-4a38-9398-844cf44ccb90")
		)
		(fp_line
			(start 1.09 1.34)
			(end 1.09 1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ec5a3ad-8775-40c3-ac27-630e1e93aa27")
		)
		(fp_line
			(start 1.09 1.47)
			(end 6.53 1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92ad9168-ad4e-424e-82b0-d864f1b33c7c")
		)
		(fp_line
			(start 1.87 -1.47)
			(end 1.87 1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa2eb8f5-f2da-44db-8651-13513edeab7c")
		)
		(fp_line
			(start 1.99 -1.47)
			(end 1.99 1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b087e230-a53b-4101-a3c9-3299aec250f7")
		)
		(fp_line
			(start 2.11 -1.47)
			(end 2.11 1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf895924-26ea-4e2c-8ccf-7848d8a04ea0")
		)
		(fp_line
			(start 6.53 -1.47)
			(end 6.53 -1.34)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a74674e0-715b-4b59-94e3-1176d111c4bf")
		)
		(fp_line
			(start 6.53 1.47)
			(end 6.53 1.34)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86a83530-dd07-4f67-8944-576e883cccd5")
		)
		(fp_rect
			(start -1.35 -1.6)
			(end 8.97 1.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "15a49c4e-1955-4ab0-be3e-6350193508e5")
		)
		(fp_line
			(start 0 0)
			(end 1.21 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d7ef59e-f5e9-457a-8640-03c095d1ca36")
		)
		(fp_line
			(start 1.89 -1.35)
			(end 1.89 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4db1548-5dde-4dca-8bae-a5e033737f4b")
		)
		(fp_line
			(start 1.99 -1.35)
			(end 1.99 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91fb80a5-7c37-4d7e-81a5-c79041097e16")
		)
		(fp_line
			(start 2.09 -1.35)
			(end 2.09 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b143f67-0fb5-43bb-9ab3-6e7c961f4be5")
		)
		(fp_line
			(start 7.62 0)
			(end 6.41 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d468f86c-afdb-4e47-9a00-10baa069c2e6")
		)
		(fp_rect
			(start 1.21 -1.35)
			(end 6.41 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "71029535-b28e-4748-90da-24e411d8067f")
		)
		(fp_text user "${REFERENCE}"
			(at 4.2 0 0)
			(layer "F.Fab")
			(uuid "b85df816-fdc8-4534-9718-10f8829ed778")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.113636)
			(net "Net-(BT1--)")
			(pinfunction "K_1")
			(pintype "passive")
			(uuid "4d8beab0-3bfd-4bec-9421-2045457d7d30")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-A)")
			(pinfunction "A_2")
			(pintype "passive")
			(uuid "64fff9ca-181e-4e79-b2c6-30056aac9d12")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(uuid "7ee46ac9-46a5-47cc-9dfb-2008c72d9672")
		(at 74.35 61.674167 180)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R3"
			(at 6.343589 2.451488 0)
			(layer "F.SilkS")
			(uuid "b206b8a7-e39b-41d4-a67e-f68d51f7f2ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100"
			(at 6.35 -3 0)
			(layer "F.Fab")
			(uuid "e0538bc1-aba7-4bab-9901-936c3d7c2c22")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.koaglobal.com/-/media/Files/KOA_Global/EN/product/commonpdf/mos.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "081635c6-3da6-450f-af21-9667a8ae2555")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cbb0ea3f-a062-44e1-b996-f33e16704e2f")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ca87dc4b-6d44-49d5-8866-ea1d2ca0679f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/579f05a1-9372-4db0-9475-0e9272b39368")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 11.66 0)
			(end 10.97 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df8bd24f-c1fc-416e-835b-2eea69a764f7")
		)
		(fp_line
			(start 1.04 0)
			(end 1.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8b82c3a3-9cf8-4b94-802e-807e10541750")
		)
		(fp_rect
			(start 1.73 -1.72)
			(end 10.97 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "dbc54c7a-30b0-40d6-8330-753208e939c5")
		)
		(fp_rect
			(start -1.05 -1.85)
			(end 13.75 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c01fc110-e3cd-4fdd-94ab-2bec8eb85155")
		)
		(fp_line
			(start 12.7 0)
			(end 10.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72298faf-e8fa-48ae-a1e8-d8b220b175a9")
		)
		(fp_line
			(start 0 0)
			(end 1.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ca93f68-b969-475f-a442-521ec368ef1b")
		)
		(fp_rect
			(start 1.85 -1.6)
			(end 10.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "af3bd252-e6fb-4776-b427-c01c30f8dd0a")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 0)
			(layer "F.Fab")
			(uuid "1e76b26d-7fc7-4b8e-a3fe-715c2973e7ca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO3")
			(pintype "passive")
			(uuid "d4edb775-3ad8-4087-8c2c-db4aa880de48")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-C)")
			(pintype "passive")
			(uuid "f90aec35-aeeb-44cd-a246-cdd4454560a1")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Battery:BatteryHolder_Keystone_2462_2xAA"
		(layer "F.Cu")
		(uuid "807b0fcd-687e-43ad-bb5f-6185cfe1d0b9")
		(at 90.835 44.005)
		(descr "2xAA cell battery holder, Keystone P/N 2462, https://www.keyelco.com/product-pdf.cfm?p=1027")
		(tags "AA battery cell holder")
		(property "Reference" "REF**"
			(at 0 -10.16 0)
			(layer "F.SilkS")
			(uuid "06dec843-c42d-4c43-a7c0-7c91d8f55835")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BatteryHolder_Keystone_2462_2xAA"
			(at 27.165 8.715 0)
			(layer "F.Fab")
			(uuid "cae9079b-521d-45db-8ca8-0514bb096d82")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e5ba4e1b-a0ff-4890-84c8-05b35b0b019c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80ffdbea-7033-4cb3-8c36-d9ce14d54a47")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -2.69 -9.065)
			(end -2.69 24.055)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d1d2d994-b6a0-4cb6-9542-d9f92639320f")
		)
		(fp_line
			(start -2.69 24.055)
			(end 57.02 24.055)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba1cc774-a739-4ef4-a519-53f96426a6d2")
		)
		(fp_line
			(start -1.42 -7.795)
			(end -1.42 22.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6a9020d-7c14-479e-8cdd-902d369aa198")
		)
		(fp_line
			(start -1.42 7.241)
			(end 55.75 7.241)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e8945a80-59a2-4d63-9890-ddfaed5f23bb")
		)
		(fp_line
			(start -1.42 22.785)
			(end 4.925 22.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "79443511-b4a3-4a84-9250-4ebbf6937635")
		)
		(fp_line
			(start 4.925 -7.795)
			(end -1.42 -7.795)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c737692-3877-449f-8048-e45e3bc51e9b")
		)
		(fp_line
			(start 4.925 -5.255)
			(end 4.925 -7.795)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "634360fc-1977-4ecc-a0d1-d265295a5932")
		)
		(fp_line
			(start 4.925 -5.255)
			(end 17.625 -5.255)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "596133a5-91e2-4d8c-8eb3-5dc7ef4e191f")
		)
		(fp_line
			(start 4.925 20.245)
			(end 17.625 20.245)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b3bd680a-6376-4f4c-9611-45593d0062d8")
		)
		(fp_line
			(start 4.925 22.785)
			(end 4.925 20.245)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9d8bd007-68ee-4e69-9a9c-d6181bfcddfa")
		)
		(fp_line
			(start 17.625 -7.795)
			(end 17.625 -5.255)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb2d016e-bdfd-4cd3-b8bb-19019cdbbc42")
		)
		(fp_line
			(start 17.625 -1.27)
			(end 18.895 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e4a2af7-3ad6-45b4-a8e3-892ed6b71a22")
		)
		(fp_line
			(start 17.625 1.27)
			(end 17.625 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6e359df9-017f-46e8-9104-af3572142317")
		)
		(fp_line
			(start 17.625 12.45)
			(end 35.405 12.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "579be95c-b257-412c-b74d-a5d49ed9569a")
		)
		(fp_line
			(start 17.625 17.53)
			(end 17.625 12.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bebd3717-3665-4d82-9a4d-7094a55c03b2")
		)
		(fp_line
			(start 17.625 20.245)
			(end 17.625 22.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "010d13c8-0cdc-4b84-9b8c-97850b4ecb73")
		)
		(fp_line
			(start 17.625 22.785)
			(end 36.675 22.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1de2da72-8e45-4f22-820d-43a2a3e5b49f")
		)
		(fp_line
			(start 18.895 -2.54)
			(end 36.675 -2.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ce944f5-52f6-495b-b3bc-849d403cbd8c")
		)
		(fp_line
			(start 18.895 -1.27)
			(end 18.895 -2.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6150c98-109e-4e6c-a6db-9355e07c4828")
		)
		(fp_line
			(start 18.895 1.27)
			(end 17.625 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "77620890-44aa-4abd-9afd-6fb3884c81ab")
		)
		(fp_line
			(start 18.895 2.54)
			(end 18.895 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "922456a5-48ab-402a-9548-c26ec7c6803f")
		)
		(fp_line
			(start 35.405 12.45)
			(end 35.405 13.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45b4f13d-b0d8-4aaf-a355-a94afde0c142")
		)
		(fp_line
			(start 35.405 13.72)
			(end 36.675 13.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b013a371-7ded-404a-ad6d-8fc08162ddbb")
		)
		(fp_line
			(start 35.405 16.26)
			(end 35.405 17.53)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f72b986-f783-4aab-b3cc-59814a6622a8")
		)
		(fp_line
			(start 35.405 17.53)
			(end 17.625 17.53)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4224d8ed-3f67-4446-a53e-800179ea64ee")
		)
		(fp_line
			(start 36.675 -7.795)
			(end 17.625 -7.795)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd4d596d-2ffb-4d17-bf25-ab867669f9a8")
		)
		(fp_line
			(start 36.675 -5.255)
			(end 36.675 -7.795)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22f4458c-c7af-4af2-9710-f10bea0682a4")
		)
		(fp_line
			(start 36.675 -2.54)
			(end 36.675 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "93ae5c53-fe92-4af8-8b0d-17c8307e6b66")
		)
		(fp_line
			(start 36.675 -1.27)
			(end 36.675 2.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dadb9971-c830-47f8-a801-a43d6981d86b")
		)
		(fp_line
			(start 36.675 2.54)
			(end 18.895 2.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7da0b8c8-f0a4-40ba-8fc8-003ea80f8f3d")
		)
		(fp_line
			(start 36.675 13.72)
			(end 36.675 16.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4aa1fae-c664-4dfe-8f65-1ae42a1e8b50")
		)
		(fp_line
			(start 36.675 16.26)
			(end 35.405 16.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ae9cc45-0e99-4bce-b838-85ea13d54d36")
		)
		(fp_line
			(start 36.675 22.785)
			(end 36.675 20.245)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68ff77ec-c757-4cc1-bce4-16ea35aa7a51")
		)
		(fp_line
			(start 49.375 -7.795)
			(end 49.375 -5.255)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "31de5722-aef8-472e-97ba-e4019a234d0c")
		)
		(fp_line
			(start 49.375 -5.255)
			(end 36.675 -5.255)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86598709-8990-4feb-8bf2-68722276c3aa")
		)
		(fp_line
			(start 49.375 20.245)
			(end 36.675 20.245)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14e51f1c-e143-45fc-9da4-894d8b525b68")
		)
		(fp_line
			(start 49.375 22.785)
			(end 49.375 20.245)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0e009993-89f9-4cb3-97e9-5e90c46e75f3")
		)
		(fp_line
			(start 55.75 -7.795)
			(end 49.375 -7.795)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f677cfd6-8c18-49d7-9837-be141e143305")
		)
		(fp_line
			(start 55.75 -7.795)
			(end 55.75 22.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f007b388-0d36-40bc-8d5d-951b1edc387f")
		)
		(fp_line
			(start 55.75 7.749)
			(end -1.42 7.749)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f76aac36-035b-4a2d-842b-c7de661abb29")
		)
		(fp_line
			(start 55.75 22.785)
			(end 49.375 22.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a7c359d-cfab-4d86-82f9-3b0684ee9972")
		)
		(fp_line
			(start 57.02 -9.065)
			(end -2.69 -9.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7efdc2d-0b05-4410-9131-75522112dd72")
		)
		(fp_line
			(start 57.02 24.055)
			(end 57.02 -9.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ec925a6-2787-4dec-8766-2f2c557ebe07")
		)
		(fp_line
			(start -2.84 -9.22)
			(end -2.84 24.21)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72b439e2-fbe7-4994-84d8-b13c33e87370")
		)
		(fp_line
			(start -2.84 24.21)
			(end 57.17 24.21)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "83f7b8d7-ee36-4726-86ac-2470b8c389c8")
		)
		(fp_line
			(start 57.17 -9.22)
			(end -2.84 -9.22)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56676a19-d0c7-4df3-8ebf-debc4b11f844")
		)
		(fp_line
			(start 57.17 24.21)
			(end 57.17 -9.22)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c51f856d-97e3-4221-955c-c1b2ca735555")
		)
		(fp_line
			(start -2.59 -8.965)
			(end 56.92 -8.965)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5d797f76-897d-46bf-b5ec-14d69357ca33")
		)
		(fp_line
			(start -2.59 23.955)
			(end -2.59 -8.965)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1bf846ef-6b4b-4ce7-b9eb-29f98fce918d")
		)
		(fp_line
			(start -2.59 23.955)
			(end 56.92 23.955)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8aeb2cf5-32ec-4f8c-80c6-4cfc9d95df9d")
		)
		(fp_line
			(start 56.92 23.955)
			(end 56.92 -8.965)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "34ac5db0-1df2-4399-8097-c375eea4d739")
		)
		(fp_text user "+"
			(at -3.81 0 0)
			(layer "F.SilkS")
			(uuid "7955a04a-31bb-4d00-aa2a-c73f5ce2b88f")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "-"
			(at -3.81 14.99 0)
			(layer "F.SilkS")
			(uuid "0f6077d1-d5f3-4c08-86e3-d484a0a426df")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "+"
			(at 16.355 0 0)
			(layer "F.SilkS")
			(uuid "cfc56d02-6b9f-4c2e-b27f-43ee502b6608")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "-"
			(at 16.355 14.99 0)
			(layer "F.SilkS")
			(uuid "ee7eb8ca-8375-47cf-b5fb-2fe66cbadfcd")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "-"
			(at 37.945 0 0)
			(layer "F.SilkS")
			(uuid "577fcb9f-3dd7-43e9-8b9e-2be19ab176a8")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "+"
			(at 37.945 14.99 0)
			(layer "F.SilkS")
			(uuid "967013c2-be51-43bd-bbaf-e8ed248abdc8")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 -10.16 0)
			(layer "F.Fab")
			(uuid "8a28c144-695e-4c0e-b6a1-4cd616fba6bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 27.165 0)
			(size 3.3 3.3)
			(drill 3.3)
			(layers "*.Cu" "*.Mask")
			(uuid "f57dd7ce-5169-4cd2-ad98-73017dd590af")
		)
		(pad "" np_thru_hole circle
			(at 27.165 14.99)
			(size 3.3 3.3)
			(drill 3.3)
			(layers "*.Cu" "*.Mask")
			(uuid "d4e86dad-c501-43cf-b073-cfb6db929f90")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "dd2ad412-59ed-4b65-9a49-e5d46218070e")
		)
		(pad "2" thru_hole circle
			(at 0 14.99)
			(size 2 2)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "97d64a87-29da-4c25-aee0-6d8088dd23f7")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_2462_2xAA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector:External Attach for Push Button"
		(layer "F.Cu")
		(uuid "85f98571-7ae5-4671-82ea-4249895bf983")
		(at 47.8375 104.5)
		(descr "THT Pads for external push button")
		(tags "external, button, placeholder")
		(property "Reference" "SW1"
			(at 0 -2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "f9579367-ff89-4a25-b32e-d896f1285849")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "SW_Push"
			(at 0 2 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "bc7c8c21-d5ce-4591-bf6d-e03f59d89e16")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "30920c75-5090-4440-a959-3f2e604e063d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "66080b00-ccf5-4b19-a44e-0dbb1eb62720")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/d4fc38fa-86cb-4463-9001-da51d2c30d89")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_rect
			(start -4 -1.5)
			(end 4 1.5)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "1735ba05-1a47-42e4-a03a-122febd347b0")
		)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(A1-GPIO16)")
			(pinfunction "1_1")
			(pintype "passive")
			(uuid "858917d3-c9e1-4e26-ae78-be58daf2216f")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "2_2")
			(pintype "passive")
			(uuid "dfafb7bc-7f49-4edf-9e21-4a25507183fb")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(uuid "8cf2a20b-a14c-46c0-b83b-0ae9d86695f0")
		(at 74.35 52.0225 180)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R1"
			(at 6.35 2.84 0)
			(layer "F.SilkS")
			(uuid "47f5fd1a-bfe2-4c8c-a72e-dd50c5e8149b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100"
			(at 6.35 -3.16 0)
			(layer "F.Fab")
			(uuid "df3c726d-c870-4eff-8e52-2e11647fb6c3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.koaglobal.com/-/media/Files/KOA_Global/EN/product/commonpdf/mos.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a49161f8-df06-4e3f-b5d4-9e262f9f3d8d")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "31d6dd12-ae5b-4fc1-92bd-6a7152efbafd")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c9a1add5-9ac4-44a4-b536-80c3559f3172")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/16d1a2ba-40fa-4e0e-8c0a-92e41cc47624")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 11.66 0)
			(end 10.97 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7f7d5a9-7595-42b9-a5fa-33f400ec0983")
		)
		(fp_line
			(start 1.04 0)
			(end 1.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "94d5482e-d682-4838-a4df-667f01eb6655")
		)
		(fp_rect
			(start 1.73 -1.72)
			(end 10.97 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "aca5ef56-4edf-45e3-8c60-ca27484c7a9f")
		)
		(fp_rect
			(start -1.05 -1.85)
			(end 13.75 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "8d930f89-cc14-41f0-bd22-4d5c0f05486a")
		)
		(fp_line
			(start 12.7 0)
			(end 10.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f3c1598a-417b-401b-b4cf-9838d73ef264")
		)
		(fp_line
			(start 0 0)
			(end 1.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a779de3-68ad-40b3-a0a5-3374261f85d3")
		)
		(fp_rect
			(start 1.85 -1.6)
			(end 10.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "4c982bec-b81b-4fe8-b3c3-286af13c2f7c")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 0)
			(layer "F.Fab")
			(uuid "234f7b9f-29c0-41e3-9172-bf1e7fd0e715")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO1")
			(pintype "passive")
			(uuid "c2e6323e-27ee-44df-82ed-573d37a61a17")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-A)")
			(pintype "passive")
			(uuid "96ed6741-5425-4856-8c75-4f9fbf2a6f30")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T_NO_CK_PTS125Sx85PSMTR"
		(layer "F.Cu")
		(uuid "8d62a66e-c1c3-4d23-8c91-a3f42778eb49")
		(at 124 78)
		(descr "Tactile switch, 12x12 mm, H8.5 mm, round actuator, with pegs, gullwing terminals, https://www.ckswitches.com/media/1462/pts125.pdf")
		(tags "button tactile switch SPST 1P1T C&K")
		(property "Reference" "REF**"
			(at 0 -7.3 0)
			(layer "F.SilkS")
			(uuid "b3751752-98a5-49d4-8f4f-d80e1904dba1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push_1P1T_NO_CK_PTS125Sx85PSMTR"
			(at 0 7.1 0)
			(layer "F.Fab")
			(uuid "ebc7641d-eb73-4758-8f81-ffae03405453")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dbf63ea8-f615-4a6d-837b-91c7de483274")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "440f09f8-a839-4b49-bb39-079c3d867e8d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -6.2 -4.6)
			(end -4.6 -6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "850a287a-7624-4411-b5e9-035cc92d0bfa")
		)
		(fp_line
			(start -6.2 -3.45)
			(end -6.2 -4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87d392c0-bc9d-4304-891d-70ea6b8ce7c8")
		)
		(fp_line
			(start -6.2 -1.55)
			(end -6.2 1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51595519-c708-4300-9676-9b8d97603631")
		)
		(fp_line
			(start -6.2 3.45)
			(end -6.2 4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb22f149-806a-4054-a477-d5dbba509e41")
		)
		(fp_line
			(start -6.2 4.6)
			(end -4.6 6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95086545-311d-46c9-a839-41631e9c8a84")
		)
		(fp_line
			(start -4.6 -6.2)
			(end 4.6 -6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2eb4667-60c8-4b64-a35c-096d2acfa792")
		)
		(fp_line
			(start -4.6 6.2)
			(end 4.6 6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cb988307-a37e-45cb-acbd-7d7cb8e331de")
		)
		(fp_line
			(start 4.6 -6.2)
			(end 6.2 -4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba4fbb45-042e-40dd-8f04-23cae033e099")
		)
		(fp_line
			(start 4.6 6.2)
			(end 6.2 4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a748bc62-7411-42ce-a41d-e06911eba601")
		)
		(fp_line
			(start 6.2 -3.45)
			(end 6.2 -4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10b66094-950d-43bd-835f-95458d128ef6")
		)
		(fp_line
			(start 6.2 -1.55)
			(end 6.2 1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a876bb50-7d90-4ce9-b58e-b5b376d180ab")
		)
		(fp_line
			(start 6.2 3.45)
			(end 6.2 4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a9f46c8-b665-40be-9025-7f2dfb763b53")
		)
		(fp_line
			(start -8.4 -6.25)
			(end 8.4 -6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "244f17d7-5c76-4421-8137-2b9c08504dd8")
		)
		(fp_line
			(start -8.4 6.25)
			(end -8.4 -6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cbf498ab-953c-424e-baac-447ca0427a83")
		)
		(fp_line
			(start 8.4 -6.25)
			(end 8.4 6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a302deb4-6ccf-4b76-859d-4695affb1900")
		)
		(fp_line
			(start 8.4 6.25)
			(end -8.4 6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6c8a99a-e242-40de-b013-930e79d741a7")
		)
		(fp_line
			(start -6 -4.5)
			(end -6 4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "66e058af-6e2e-4abb-b212-0088459ffa09")
		)
		(fp_line
			(start -6 -4.5)
			(end -4.5 -6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81bee52e-cd22-403c-a75d-174de240445a")
		)
		(fp_line
			(start -4.5 6)
			(end -6 4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f20cc95-7273-4464-9423-0d242331dc5f")
		)
		(fp_line
			(start -4.5 6)
			(end 4.5 6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f50412d-3a1d-48fe-978b-a73d0e0834dc")
		)
		(fp_line
			(start 4.5 -6)
			(end -4.5 -6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57657a87-bb9d-45a7-bc65-44d2c15118a9")
		)
		(fp_line
			(start 4.5 -6)
			(end 6 -4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "908dbbf0-9154-4e62-a796-a2ad8e5962bc")
		)
		(fp_line
			(start 6 4.5)
			(end 4.5 6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d32084cf-5963-4b67-834d-1f6a8675f4b7")
		)
		(fp_line
			(start 6 4.5)
			(end 6 -4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9dad4092-049f-4527-8737-84a234f5e1ec")
		)
		(fp_circle
			(center 0 0)
			(end 3.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "6e9e519d-f64a-481b-a0cf-731f5b58291f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6ab78aec-8fc2-41f7-927f-1907f45b5a5a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 -4.5)
			(size 2 2)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(uuid "ff1161fe-86d9-48d6-9717-6638dc19ef9d")
		)
		(pad "" np_thru_hole circle
			(at 0 4.5)
			(size 2 2)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(uuid "9bfbe00a-ce53-40c6-9e0f-ea759c314663")
		)
		(pad "1" smd roundrect
			(at -7.15 -2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "a5435c5d-196a-4e03-81e6-d2b1abb6d857")
		)
		(pad "1" smd roundrect
			(at 7.15 -2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "227732ae-bf72-4fdf-b27b-7fd76e3d146f")
		)
		(pad "2" smd roundrect
			(at -7.15 2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "716d7f09-c644-457c-9865-c93cb7fab28a")
		)
		(pad "2" smd roundrect
			(at 7.15 2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "7389ffeb-a648-4833-9fea-5d6a8076fd8a")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_CK_PTS125Sx85PSMTR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T_NO_CK_PTS125Sx85PSMTR"
		(layer "F.Cu")
		(uuid "9cdb9268-474b-4897-9247-4e07df9475b7")
		(at 124 92)
		(descr "Tactile switch, 12x12 mm, H8.5 mm, round actuator, with pegs, gullwing terminals, https://www.ckswitches.com/media/1462/pts125.pdf")
		(tags "button tactile switch SPST 1P1T C&K")
		(property "Reference" "REF**"
			(at 0 -7.3 0)
			(layer "F.SilkS")
			(uuid "e2e50d5c-8182-4987-b4ae-7fa14f7b47ea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push_1P1T_NO_CK_PTS125Sx85PSMTR"
			(at 0 7.1 0)
			(layer "F.Fab")
			(uuid "753c0822-5b97-4589-870f-e7375315598f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1285bb7e-7f65-45e8-be39-68d7ac4899d4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c7388456-e86b-4a37-9811-4d2348e9fbdc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -6.2 -4.6)
			(end -4.6 -6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cc066499-360e-4fbf-bbd8-c5fc6b3d0caf")
		)
		(fp_line
			(start -6.2 -3.45)
			(end -6.2 -4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8644c98f-5e4b-4544-a52f-42868a48b22d")
		)
		(fp_line
			(start -6.2 -1.55)
			(end -6.2 1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32eca67b-fb38-4156-a2e7-a834255356b6")
		)
		(fp_line
			(start -6.2 3.45)
			(end -6.2 4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "70f47db6-5df1-40a6-a79d-e674adb1e7bb")
		)
		(fp_line
			(start -6.2 4.6)
			(end -4.6 6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4eab01a0-31d4-4d71-b795-1739b4154df3")
		)
		(fp_line
			(start -4.6 -6.2)
			(end 4.6 -6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7aadbc20-5457-452e-8a66-06baa83234c5")
		)
		(fp_line
			(start -4.6 6.2)
			(end 4.6 6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8207d3db-7ba7-4db7-b174-ab44b09583aa")
		)
		(fp_line
			(start 4.6 -6.2)
			(end 6.2 -4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "69b7808c-4323-40a7-b70d-f4d344935120")
		)
		(fp_line
			(start 4.6 6.2)
			(end 6.2 4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f9c831f-0503-487b-ba95-f119bf819172")
		)
		(fp_line
			(start 6.2 -3.45)
			(end 6.2 -4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc09cfab-ae84-430f-bb61-828de5e30343")
		)
		(fp_line
			(start 6.2 -1.55)
			(end 6.2 1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9eddc0ff-021a-49a3-a4f2-82a459e99a0f")
		)
		(fp_line
			(start 6.2 3.45)
			(end 6.2 4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c2220122-e80d-4d40-af69-39f24c4fdfb6")
		)
		(fp_line
			(start -8.4 -6.25)
			(end 8.4 -6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "543f0aa6-84cc-49bc-81c0-96ab74c6ac85")
		)
		(fp_line
			(start -8.4 6.25)
			(end -8.4 -6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12007adb-e908-43bd-8c61-4fedb05011ea")
		)
		(fp_line
			(start 8.4 -6.25)
			(end 8.4 6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db4ceaf7-5c72-4b20-b2e2-ca9182257e23")
		)
		(fp_line
			(start 8.4 6.25)
			(end -8.4 6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "541f181e-026e-48f9-a528-b147eb7f2afa")
		)
		(fp_line
			(start -6 -4.5)
			(end -6 4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c594e7ec-298f-4f54-9af8-a0c4b21dbd40")
		)
		(fp_line
			(start -6 -4.5)
			(end -4.5 -6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "501be833-2cb0-4eaa-a819-c3b062ad6034")
		)
		(fp_line
			(start -4.5 6)
			(end -6 4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56f3140a-f0d1-4a61-bd7b-430fc5e22a5e")
		)
		(fp_line
			(start -4.5 6)
			(end 4.5 6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "399e0657-003b-47b2-a89f-b66b8e1647ce")
		)
		(fp_line
			(start 4.5 -6)
			(end -4.5 -6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2bfc48f-43d0-4ca5-8fb5-da05f6e07dd9")
		)
		(fp_line
			(start 4.5 -6)
			(end 6 -4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "afa3249d-ee7f-42ba-9fd9-39de325fd590")
		)
		(fp_line
			(start 6 4.5)
			(end 4.5 6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "548f1eed-5aa2-40e2-91a8-8b777cdee48c")
		)
		(fp_line
			(start 6 4.5)
			(end 6 -4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d312be5f-b9a8-47f5-ae34-b5d356e67c42")
		)
		(fp_circle
			(center 0 0)
			(end 3.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "1b315d65-1fea-42ee-9006-662ea709b892")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "219b5e11-0661-49d7-8587-1565e98589ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 -4.5)
			(size 2 2)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(uuid "710a0f45-4b88-4f3e-8528-7582d56cf320")
		)
		(pad "" np_thru_hole circle
			(at 0 4.5)
			(size 2 2)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(uuid "4d72b67b-4388-4338-9252-4e1a8a896c6c")
		)
		(pad "1" smd roundrect
			(at -7.15 -2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "5d4dcbfb-4495-4f96-9589-361a92fffb91")
		)
		(pad "1" smd roundrect
			(at 7.15 -2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "db09cc80-94e7-4fe0-b59e-c890b2594716")
		)
		(pad "2" smd roundrect
			(at -7.15 2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "e4276177-bad2-480e-9a59-4c4d3a4dc36b")
		)
		(pad "2" smd roundrect
			(at 7.15 2.5)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(uuid "bb6e0b34-f2c3-47de-9a1c-724927f80645")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_CK_PTS125Sx85PSMTR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector:External Attach for Push Button"
		(layer "F.Cu")
		(uuid "b60a0250-2989-421f-910d-6ee64f560794")
		(at 47.8375 96.5)
		(descr "THT Pads for external push button")
		(tags "external, button, placeholder")
		(property "Reference" "SW3"
			(at 0 -2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "66e70689-c507-4be4-ac32-45bbdaffdd6e")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "SW_Push"
			(at 0 2 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "bc5aa6d8-c409-4ed3-9deb-430a358a2503")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7ff09e99-05a3-4f6e-85a0-67878c62b208")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "995b36b5-21e0-482b-9368-0ff3eb1e65ea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/689058f8-6732-41d3-891c-925fbabd8ebe")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_rect
			(start -4 -1.5)
			(end 4 1.5)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "3a5db6a3-20ed-400e-807f-99a9739455b0")
		)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(A1-GPIO18)")
			(pinfunction "1_1")
			(pintype "passive")
			(uuid "396b1965-f742-449e-9bf8-3380538e0e5a")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "2_2")
			(pintype "passive")
			(uuid "8c286d77-889c-47d1-acc7-f35c400082d9")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(uuid "ba8e7651-18c0-4485-ab28-2770730d33bb")
		(at 74.35 66.5 180)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R8"
			(at 6.328732 2.474213 0)
			(layer "F.SilkS")
			(uuid "3039e968-37ce-405a-8951-cd1ec333e7d2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100"
			(at 6.35 -3 0)
			(layer "F.Fab")
			(uuid "094a01dd-9f85-4c80-b5ae-4c14cc6d1d77")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.koaglobal.com/-/media/Files/KOA_Global/EN/product/commonpdf/mos.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6cad9cec-c24c-46a3-994c-dcd39bf099b0")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4d9a527c-1484-49c1-a31c-379a301d7344")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7052c49e-5c1f-4201-a200-5f46d192ea30")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0131a837-349e-4ab2-8160-fd677d4d9f42")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 11.66 0)
			(end 10.97 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2dc2bf70-21ac-438e-a376-60079774c8c9")
		)
		(fp_line
			(start 1.04 0)
			(end 1.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c78e3a99-25ee-4975-b480-7b4853a6137f")
		)
		(fp_rect
			(start 1.73 -1.72)
			(end 10.97 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "a94b2983-e3be-4ac2-82ae-84b7b0a58358")
		)
		(fp_rect
			(start -1.05 -1.85)
			(end 13.75 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "45398445-c0bd-4f77-895f-fe67aab195cd")
		)
		(fp_line
			(start 12.7 0)
			(end 10.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f92754ba-50ea-4523-a81a-4e6556fac988")
		)
		(fp_line
			(start 0 0)
			(end 1.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6262725b-cfea-4f06-8de1-c236a87e1106")
		)
		(fp_rect
			(start 1.85 -1.6)
			(end 10.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "53903d1a-17c4-4adf-ab37-734183bf6df5")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 0)
			(layer "F.Fab")
			(uuid "b46648f5-0a9c-4720-a5aa-aa58b1d51950")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO4")
			(pintype "passive")
			(uuid "f3d4e608-1e5c-4e9e-9f81-18c2ee3523f4")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-DP)")
			(pintype "passive")
			(uuid "0b0cd0c1-8ddd-4093-938e-4b91e30599c9")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(uuid "cb4ef212-54db-411b-b76e-0c4aae55a792")
		(at 74.35 56.848333 180)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R2"
			(at 6.328732 2.547623 0)
			(layer "F.SilkS")
			(uuid "523b47b7-dd1a-4a62-8feb-c14c7d1ae1c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100"
			(at 6.35 -3 0)
			(layer "F.Fab")
			(uuid "e2eb981f-27dd-42ba-831e-5b8c4f792275")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.koaglobal.com/-/media/Files/KOA_Global/EN/product/commonpdf/mos.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d9eb5024-ad01-48d2-9a00-cb76da048ac6")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "88b63d69-8c17-4070-9cee-f7f886ee96d6")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "1bd79b4d-f56b-44e3-b419-4d380880fc8e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/08048f86-eca9-4105-b550-9be7db6459ed")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 11.66 0)
			(end 10.97 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af45f9e4-1326-4751-9dbe-6e38f4a366d5")
		)
		(fp_line
			(start 1.04 0)
			(end 1.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9db5b176-668f-4b39-a293-7ca0cde54b8c")
		)
		(fp_rect
			(start 1.73 -1.72)
			(end 10.97 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "63a49232-cb51-4e4d-b9b1-f38718187b0a")
		)
		(fp_rect
			(start -1.05 -1.85)
			(end 13.75 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "0953ae8f-58b0-415f-8662-27e38f710f0a")
		)
		(fp_line
			(start 12.7 0)
			(end 10.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e39df6f6-b12a-4e55-8d25-c17744815d05")
		)
		(fp_line
			(start 0 0)
			(end 1.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87cd4465-016d-401c-ab11-ad275bd2921e")
		)
		(fp_rect
			(start 1.85 -1.6)
			(end 10.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "36c78d9f-84a0-44f0-92e7-a3bbfbcbe772")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 0)
			(layer "F.Fab")
			(uuid "c7cfee16-5e1b-474c-83dc-786a814059b1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO2")
			(pintype "passive")
			(uuid "5456033f-ba7b-4431-99a5-65834b474a27")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-B)")
			(pintype "passive")
			(uuid "d09b9d7c-b85f-4702-ad1c-02a2ea595373")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(uuid "d3817ad9-7578-4e3e-870a-a014bf769af5")
		(at 35.0975 66.5)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R4"
			(at 6.35 -2.72 0)
			(layer "F.SilkS")
			(uuid "bc0c1af6-73c9-4ae7-abde-7af22c6ee553")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100"
			(at 6.35 2.72 0)
			(layer "F.Fab")
			(uuid "96ed777c-a1a1-456e-b908-d49db23e4370")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.koaglobal.com/-/media/Files/KOA_Global/EN/product/commonpdf/mos.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e2135a4e-9d6e-4d7d-88d0-710cd9a6a7b5")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cfbf6286-7e04-4568-b3a4-26c4221ea546")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "306a7b91-d03b-4e50-a0a2-8c28822cf53a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/23a1c513-b366-438c-b097-bbc1ee29f3af")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 1.04 0)
			(end 1.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84cf28e6-fe25-4cd4-84e5-11b3e08491e9")
		)
		(fp_line
			(start 11.66 0)
			(end 10.97 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "80c34b7a-60d3-42a4-b428-1fd69d617d95")
		)
		(fp_rect
			(start 1.73 -1.72)
			(end 10.97 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "05c21f3a-aa01-4532-9ea1-ca54681dd3fd")
		)
		(fp_rect
			(start -1.05 -1.85)
			(end 13.75 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "08a716b9-cdc4-4890-a2c7-20437b0afeeb")
		)
		(fp_line
			(start 0 0)
			(end 1.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b437593-bd87-49a8-b52d-48c872b9fe8f")
		)
		(fp_line
			(start 12.7 0)
			(end 10.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b1e60b9-3e08-4adb-91b0-25889d334529")
		)
		(fp_rect
			(start 1.85 -1.6)
			(end 10.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "18c35dac-8329-4ecc-a3b1-541bad618a4b")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 0)
			(layer "F.Fab")
			(uuid "59ee43ef-ea22-492a-8bdf-0a1bb61ef2a4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO8")
			(pintype "passive")
			(uuid "695a5767-1f72-4c7a-bcb1-c1deae19f3ab")
		)
		(pad "2" thru_hole circle
			(at 12.7 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-D)")
			(pintype "passive")
			(uuid "1143e126-e6f6-4039-b832-294e9709c0fe")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Display_7Segment:HDSP-A151"
		(layer "F.Cu")
		(uuid "f759fc4b-25d1-41e8-9775-0c368e6a6abc")
		(at 52.0325 54.4825)
		(descr "One digit 7 segment red, https://docs.broadcom.com/docs/AV02-2553EN")
		(tags "One digit 7 segment high efficiency red")
		(property "Reference" "U2"
			(at 2.54 -2.159 0)
			(layer "F.SilkS")
			(uuid "b4a92a2a-2349-4ee3-857b-ef8f45649f94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "HDSP-7501"
			(at 2.54 12.7 0)
			(layer "F.Fab")
			(uuid "65083f19-f80d-4395-b9f7-75b5f73cac8a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9468c6db-0e7a-4bb7-ac12-98a54725b3f7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "One digit 7 segment high efficiency red, common anode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd214ab4-51dc-44a6-91d1-1391f96a7b06")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "HDSP?A151*")
		(path "/f8bfa67a-939c-4399-b8e2-588d22421405")
		(sheetname "/")
		(sheetfile "kuulutusjärjestelmä.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "10" "9" "8" "5" "4" "2" "3" "7" "1" "6")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.63 -1.63)
			(end 0 -1.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dbe3f3c6-a0a2-4d15-ad4f-aabd8a54fb60")
		)
		(fp_line
			(start -1.63 0)
			(end -1.63 -1.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c2ea94d5-476f-4756-9955-e95a0cde0f89")
		)
		(fp_line
			(start -1.27 -1.27)
			(end -1.27 11.43)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a7fd0cf-d9d7-45a4-8b41-4f8110a5bd03")
		)
		(fp_line
			(start -1.27 11.43)
			(end 6.35 11.43)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7bd412cc-def8-4590-ade6-1434c404914b")
		)
		(fp_line
			(start 6.35 -1.27)
			(end -1.27 -1.27)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "adb3fdee-1e61-4b2b-b0c6-162392a87c4a")
		)
		(fp_line
			(start 6.35 11.43)
			(end 6.35 -1.27)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26fc0761-a785-4dcb-b63e-fe00b5be1d11")
		)
		(fp_line
			(start -1.5 -1.5)
			(end 6.6 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a895a28a-e302-410b-a6ed-30a4b52fbf1a")
		)
		(fp_line
			(start -1.5 11.7)
			(end -1.5 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d196942-430d-48ad-b4f2-9752a74cbe2c")
		)
		(fp_line
			(start 6.6 -1.5)
			(end 6.6 11.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ad8789b-7b81-43f7-9ab3-8fe02de8ad5f")
		)
		(fp_line
			(start 6.6 11.7)
			(end -1.5 11.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "448d76e4-91ca-4819-a74e-04a667f4675a")
		)
		(fp_line
			(start -1.1 -0.1)
			(end -0.1 -1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "146195c1-5384-4312-ac10-b06e83be1990")
		)
		(fp_line
			(start -1.1 11.3)
			(end -1.1 -0.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b53744f2-00d1-4eab-bb80-78e6a14e3e3e")
		)
		(fp_line
			(start -0.1 -1.1)
			(end 6.2 -1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ffba463-431a-4fce-bb4b-e57adcd2b1ba")
		)
		(fp_line
			(start 6.2 -1.1)
			(end 6.2 11.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b5eb007-d358-47f8-b815-bc8e43e59d04")
		)
		(fp_line
			(start 6.2 11.3)
			(end -1.1 11.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8df0ed8f-e91c-4d37-b8ba-b7409281eef9")
		)
		(fp_text user "${REFERENCE}"
			(at 2.573 5.08 0)
			(layer "F.Fab")
			(uuid "7f73879f-3308-4fd5-bb3a-7d1ca0f882b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO9")
			(pinfunction "CA_1")
			(pintype "input")
			(uuid "25154f5a-7038-47c6-bcc0-de50d2ff015b")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-F)")
			(pinfunction "F_2")
			(pintype "input")
			(uuid "f45c43d4-52be-4a11-b08c-f8b8931cfb8e")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-G)")
			(pinfunction "G_3")
			(pintype "input")
			(uuid "4a6f9530-dc57-4e53-8ac9-585a6cf841dc")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-E)")
			(pinfunction "E_4")
			(pintype "input")
			(uuid "940786e1-34b8-4536-b5a2-3168aeb611b4")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-D)")
			(pinfunction "D_5")
			(pintype "input")
			(uuid "ba385541-5d75-4814-ba49-385dce7525a2")
		)
		(pad "6" thru_hole circle
			(at 5.08 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/GPIO0")
			(pinfunction "CA_6")
			(pintype "input")
			(uuid "c80e36ca-50c4-42f7-84b3-503d5e5dbed7")
		)
		(pad "7" thru_hole circle
			(at 5.08 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-DP)")
			(pinfunction "DP_7")
			(pintype "input")
			(uuid "9597687d-e200-4a0a-9a64-6d1152497d3d")
		)
		(pad "8" thru_hole circle
			(at 5.08 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-C)")
			(pinfunction "C_8")
			(pintype "input")
			(uuid "afc7bad6-3dfe-4540-b830-96d0d7e5a9ef")
		)
		(pad "9" thru_hole circle
			(at 5.08 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-B)")
			(pinfunction "B_9")
			(pintype "input")
			(uuid "4a6591ae-4eb0-4615-8941-147b244ac7b9")
		)
		(pad "10" thru_hole circle
			(at 5.08 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-A)")
			(pinfunction "A_10")
			(pintype "input")
			(uuid "27009a9b-0fed-403d-89f4-374d8c87b6d1")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Display_7Segment.3dshapes/HDSP-A151.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 29.5 48.5)
		(end 83 108.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "00b065d1-795e-437c-83bc-66876b150d65")
	)
	(gr_text "-"
		(at 68.5 104.232571 -180)
		(layer "F.SilkS")
		(uuid "3c606608-3844-4aca-b4f0-547adbb67bf0")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "+"
		(at 75 104 270)
		(layer "F.SilkS")
		(uuid "4dfda5b7-5072-40e6-8c88-696ad3069f9e")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(segment
		(start 37.5 54.425)
		(end 35.0975 52.0225)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO5")
		(uuid "123a0c11-cede-41d7-ae54-85ace74973c2")
	)
	(segment
		(start 37.5 59)
		(end 37.5 54.425)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO5")
		(uuid "40d34e1a-4019-4e8d-8861-d5650cfa1dd7")
	)
	(segment
		(start 47.5 69)
		(end 37.5 59)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO5")
		(uuid "66e55cfb-25c5-48a8-b50a-372aca6e7d67")
	)
	(segment
		(start 65.5775 74)
		(end 60.5775 69)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO5")
		(uuid "8ec914e2-4373-459d-a908-08e165c3e741")
	)
	(segment
		(start 60.5775 69)
		(end 47.5 69)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO5")
		(uuid "eac2b81d-5eab-45d4-a1c2-690bb465ed26")
	)
	(segment
		(start 51.0225 57.0225)
		(end 52.0325 57.0225)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-F)")
		(uuid "06f6b3d3-96f8-48b8-a82a-66329e0eac6d")
	)
	(segment
		(start 47.7975 53.7975)
		(end 51.0225 57.0225)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-F)")
		(uuid "57f2d25e-de6c-402b-98e7-c24ac69f41aa")
	)
	(segment
		(start 47.7975 52.0225)
		(end 47.7975 53.7975)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-F)")
		(uuid "f0d2de9d-f6a6-4e35-8f09-ce1d6b7e161e")
	)
	(segment
		(start 46 70)
		(end 35.0975 59.0975)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO6")
		(uuid "22381053-fd02-4088-8093-da1d714145d1")
	)
	(segment
		(start 56.4975 70)
		(end 46 70)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO6")
		(uuid "254d79be-3409-4d09-ba3f-655043815975")
	)
	(segment
		(start 35.0975 59.0975)
		(end 35.0975 56.848333)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO6")
		(uuid "6206ae32-0fe0-46ea-a8a5-d622fd8fe08e")
	)
	(segment
		(start 60.4975 74)
		(end 56.4975 70)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO6")
		(uuid "fcd055bb-8781-4bd2-bef3-d9e4a20e6944")
	)
	(segment
		(start 47.7975 56.848333)
		(end 47.7975 57.7975)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-G)")
		(uuid "0000baf7-219a-4d06-9fa6-77e37c2b2c8d")
	)
	(segment
		(start 47.7975 57.7975)
		(end 49.5625 59.5625)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-G)")
		(uuid "a209a027-b519-4a76-8471-d5295f060b46")
	)
	(segment
		(start 49.5625 59.5625)
		(end 52.0325 59.5625)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-G)")
		(uuid "e7b843c5-ad1d-4e6c-a3e0-db09abe55f54")
	)
	(segment
		(start 35.0975 63.0975)
		(end 35.0975 61.674167)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO7")
		(uuid "334d4831-941a-4d48-8add-c7ba1dade9b0")
	)
	(segment
		(start 43 71)
		(end 35.0975 63.0975)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO7")
		(uuid "a5d0e20d-3a03-4b4f-b250-aab8fc087345")
	)
	(segment
		(start 57.9575 74)
		(end 54.9575 71)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO7")
		(uuid "e12a1bbc-c366-400d-9b58-00728a04f37c")
	)
	(segment
		(start 54.9575 71)
		(end 43 71)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO7")
		(uuid "ecc8c67c-ea77-412d-ba52-f515b39e71ec")
	)
	(segment
		(start 50.1025 62.1025)
		(end 52.0325 62.1025)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-E)")
		(uuid "10acedb4-ff35-436a-a8c3-18fcced10559")
	)
	(segment
		(start 47.7975 61.674167)
		(end 49.674167 61.674167)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-E)")
		(uuid "2797b80f-4021-4a08-908c-54f4349497dc")
	)
	(segment
		(start 49.674167 61.674167)
		(end 50.1025 62.1025)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-E)")
		(uuid "5717be1f-43e6-41e0-a8ca-e1ddcd188d73")
	)
	(segment
		(start 69 97)
		(end 63.81 97)
		(width 0.8)
		(layer "F.Cu")
		(net "Net-(D1-A)")
		(uuid "a5a259b5-b1e1-4330-a73b-549259fd9803")
	)
	(segment
		(start 50.3375 104.5)
		(end 50.3375 100.5)
		(width 0.4)
		(layer "F.Cu")
		(net "GND")
		(uuid "1ce2bef1-bfe9-4d24-bc52-c99ccb22e799")
	)
	(segment
		(start 75.7375 95.2625)
		(end 75.7375 91.78)
		(width 0.8)
		(layer "F.Cu")
		(net "GND")
		(uuid "42ac35e5-5965-4421-a98a-be06c14a32f0")
	)
	(segment
		(start 50.3375 100.5)
		(end 50.3375 96.5)
		(width 0.4)
		(layer "F.Cu")
		(net "GND")
		(uuid "95d18788-c669-4832-a357-987055291126")
	)
	(segment
		(start 74 97)
		(end 75.7375 95.2625)
		(width 0.8)
		(layer "F.Cu")
		(net "GND")
		(uuid "be893cff-9c6d-4bec-816b-9fa08f67eaea")
	)
	(segment
		(start 50.3375 96.5)
		(end 50.3375 91.78)
		(width 0.4)
		(layer "F.Cu")
		(net "GND")
		(uuid "f6012e71-4271-4ef0-b8f9-5fe792ba29f1")
	)
	(segment
		(start 45.3375 100.5)
		(end 42 100.5)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(A1-GPIO17)")
		(uuid "3e039d3e-b02f-4887-9b5c-dd8fa583eeef")
	)
	(segment
		(start 35.0975 93.5975)
		(end 35.0975 91.78)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(A1-GPIO17)")
		(uuid "aaaa3867-4b95-4c88-8217-d61760925c91")
	)
	(segment
		(start 42 100.5)
		(end 35.0975 93.5975)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(A1-GPIO17)")
		(uuid "be75bc26-01ab-40c1-9446-e6f6ae5244e7")
	)
	(segment
		(start 60 70)
		(end 57.1125 67.1125)
		(width 0.4)
		(layer "B.Cu")
		(net "/GPIO0")
		(uuid "0e4991c2-256e-4f0c-ae00-9e426c49a001")
	)
	(segment
		(start 76.8175 70)
		(end 60 70)
		(width 0.4)
		(layer "B.Cu")
		(net "/GPIO0")
		(uuid "6d3b2e2e-54a6-4b98-b94c-60ac90f70df5")
	)
	(segment
		(start 80.8175 74)
		(end 76.8175 70)
		(width 0.4)
		(layer "B.Cu")
		(net "/GPIO0")
		(uuid "730f99d9-5d18-407c-85d9-a35ab93d7e18")
	)
	(segment
		(start 57.1125 67.1125)
		(end 57.1125 64.6425)
		(width 0.4)
		(layer "B.Cu")
		(net "/GPIO0")
		(uuid "c3f1a7fa-3113-4ece-a921-4705229633fa")
	)
	(segment
		(start 78.2775 74)
		(end 78.2775 71.2225)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO1")
		(uuid "28918e4a-bf84-47ef-b89b-f5006d240aeb")
	)
	(segment
		(start 79.5 70)
		(end 79.5 55)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO1")
		(uuid "73b9b46f-2af8-4b19-953b-cf4b4e704105")
	)
	(segment
		(start 78.2775 71.2225)
		(end 79.5 70)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO1")
		(uuid "a920f58f-286e-444a-a5de-50096016fa06")
	)
	(segment
		(start 76.5225 52.0225)
		(end 74.35 52.0225)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO1")
		(uuid "acda3fb1-0932-45ed-a04f-a9656c56bcc7")
	)
	(segment
		(start 79.5 55)
		(end 76.5225 52.0225)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO1")
		(uuid "d8e28306-e855-4ff8-88fa-fbce94c1eef1")
	)
	(segment
		(start 76.348333 56.848333)
		(end 74.35 56.848333)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO2")
		(uuid "6db5fa59-2521-48b4-97cf-eb7f1b9ec14b")
	)
	(segment
		(start 78 69.1975)
		(end 78 58.5)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO2")
		(uuid "821e2e7c-5fab-4158-96c0-804c4fa4f98a")
	)
	(segment
		(start 73.1975 74)
		(end 78 69.1975)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO2")
		(uuid "8b3c4382-ad17-450b-8eb1-90504b947809")
	)
	(segment
		(start 78 58.5)
		(end 76.348333 56.848333)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO2")
		(uuid "bed8c40e-bbf1-4ebb-a4d4-5fbcc17fdbdc")
	)
	(segment
		(start 76.5 63.824167)
		(end 74.35 61.674167)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO3")
		(uuid "a9ea8fb1-381d-4ab5-a0ae-361f878f23a6")
	)
	(segment
		(start 76.5 68.1575)
		(end 76.5 63.824167)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO3")
		(uuid "babb45d9-cf7f-40bd-8b30-bb16bdd60cf7")
	)
	(segment
		(start 70.6575 74)
		(end 76.5 68.1575)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO3")
		(uuid "f38d4e5c-d36b-4aae-af66-290d0cd8faf4")
	)
	(segment
		(start 68.1175 72.7325)
		(end 74.35 66.5)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO4")
		(uuid "54bab38f-1279-48f0-87ea-e53b6fe4765e")
	)
	(segment
		(start 68.1175 74)
		(end 68.1175 72.7325)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO4")
		(uuid "deb8fab8-2da7-4d3d-ab70-11336fa30f09")
	)
	(segment
		(start 40.5975 72)
		(end 35.0975 66.5)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO8")
		(uuid "0ed3d012-64b3-4037-b391-fa39e786e76b")
	)
	(segment
		(start 53.4175 72)
		(end 40.5975 72)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO8")
		(uuid "9902f930-5dc4-4057-a0f1-9dd9d6448469")
	)
	(segment
		(start 55.4175 74)
		(end 53.4175 72)
		(width 0.4)
		(layer "F.Cu")
		(net "/GPIO8")
		(uuid "ae72e780-dcec-461d-94b0-242527ae38bb")
	)
	(segment
		(start 54.5 72.3775)
		(end 54.5 55.5)
		(width 0.4)
		(layer "B.Cu")
		(net "/GPIO9")
		(uuid "3bf09391-0c98-457e-aec0-f49135f40de7")
	)
	(segment
		(start 53.4825 54.4825)
		(end 52.0325 54.4825)
		(width 0.4)
		(layer "B.Cu")
		(net "/GPIO9")
		(uuid "650b4739-04d3-4506-af50-14ad449a00c2")
	)
	(segment
		(start 52.8775 74)
		(end 54.5 72.3775)
		(width 0.4)
		(layer "B.Cu")
		(net "/GPIO9")
		(uuid "930ea8f6-81b6-4ca6-8583-c13d640a16b9")
	)
	(segment
		(start 54.5 55.5)
		(end 53.4825 54.4825)
		(width 0.4)
		(layer "B.Cu")
		(net "/GPIO9")
		(uuid "c2ca29d4-26a7-41a8-a21f-979312361d56")
	)
	(segment
		(start 45.3375 104.5)
		(end 43.5 104.5)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(A1-GPIO16)")
		(uuid "513770db-79b6-4a52-9350-f1ea5dab4b24")
	)
	(segment
		(start 43.5 104.5)
		(end 32.5575 93.5575)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(A1-GPIO16)")
		(uuid "b469f0c5-2402-4d7a-853b-c34cd8237f88")
	)
	(segment
		(start 32.5575 93.5575)
		(end 32.5575 91.78)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(A1-GPIO16)")
		(uuid "c5eb833b-051c-4b39-acf4-c752053aee78")
	)
	(segment
		(start 40.1775 93.6775)
		(end 40.1775 91.78)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(A1-GPIO18)")
		(uuid "5329e4f0-f982-4f53-b62e-206d75b8286c")
	)
	(segment
		(start 45.3375 96.5)
		(end 43 96.5)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(A1-GPIO18)")
		(uuid "d24cdae3-a067-4b3b-8a86-75eb2cf5e8b6")
	)
	(segment
		(start 43 96.5)
		(end 40.1775 93.6775)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(A1-GPIO18)")
		(uuid "f053c27c-82b9-4d6a-9b74-9a1e7543808b")
	)
	(segment
		(start 78.2775 98.7225)
		(end 78.2775 91.78)
		(width 0.8)
		(layer "F.Cu")
		(net "Net-(A1-VSYS)")
		(uuid "1a066b19-385a-4999-b86f-b5c696c1a7be")
	)
	(segment
		(start 74 103)
		(end 78.2775 98.7225)
		(width 0.8)
		(layer "F.Cu")
		(net "Net-(A1-VSYS)")
		(uuid "dacc3769-3a41-4d27-84fa-befe3e494778")
	)
	(segment
		(start 69 103)
		(end 62.19 103)
		(width 0.8)
		(layer "F.Cu")
		(net "Net-(BT1--)")
		(uuid "006a70f2-8ec6-4f65-ba5e-5be856297f5c")
	)
	(segment
		(start 62.19 103)
		(end 56.19 97)
		(width 0.8)
		(layer "F.Cu")
		(net "Net-(BT1--)")
		(uuid "9f616635-fa31-4809-a807-55d0f4aa4611")
	)
	(segment
		(start 61.65 61.674167)
		(end 59.538333 59.5625)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-C)")
		(uuid "4bfdca26-4403-401b-ade6-5093c9805456")
	)
	(segment
		(start 59.538333 59.5625)
		(end 57.1125 59.5625)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-C)")
		(uuid "ee8795da-b475-4fef-b456-318d0c14b6a1")
	)
	(segment
		(start 59.5725 52.0225)
		(end 57.1125 54.4825)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-A)")
		(uuid "c54d9eb9-625e-44e5-9389-78aacd8c3079")
	)
	(segment
		(start 61.65 52.0225)
		(end 59.5725 52.0225)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-A)")
		(uuid "f3fdb4ee-ba01-4c49-9a6b-c629b83367f2")
	)
	(segment
		(start 61.65 65.15)
		(end 58.6025 62.1025)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-DP)")
		(uuid "1cdffec5-2212-46a1-9a77-f01b62bbd20a")
	)
	(segment
		(start 61.65 66.5)
		(end 61.65 65.15)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-DP)")
		(uuid "36679b25-cd02-4188-96f0-342722e77305")
	)
	(segment
		(start 58.6025 62.1025)
		(end 57.1125 62.1025)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-DP)")
		(uuid "528a9964-fe2a-4a0c-86ec-0aa3414fce86")
	)
	(segment
		(start 59.4775 57.0225)
		(end 57.1125 57.0225)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-B)")
		(uuid "54bd8f5f-4b1e-4f25-8627-80e38f65299a")
	)
	(segment
		(start 61.65 56.848333)
		(end 59.651667 56.848333)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-B)")
		(uuid "c0398246-a6bf-4964-860d-c4ab3104ac39")
	)
	(segment
		(start 59.651667 56.848333)
		(end 59.4775 57.0225)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-B)")
		(uuid "d1e10f60-e063-441e-ad98-ffc691c8f7a4")
	)
	(segment
		(start 52.0325 64.6425)
		(end 49.655 64.6425)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-D)")
		(uuid "5f88e75f-276d-476e-8dc0-f2fbf9e5c226")
	)
	(segment
		(start 49.655 64.6425)
		(end 47.7975 66.5)
		(width 0.4)
		(layer "F.Cu")
		(net "Net-(U2-D)")
		(uuid "fa2efece-4d4b-42e0-bba3-ea15d176363f")
	)
	(embedded_fonts no)
)
