(footprint "RaspberryPi_Pico_PinSocket_1x20_P2.54mm_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Through hole straight socket strip for individual placement alongside a virtual Raspberry Pi Pico, 1x20, 2.54mm pitch, single row, default socket model has height of 8.51mm")
	(tags "Raspberry Pi Pico through hole socket strip THT 1x20 2.54mm single row")
	(property "Reference" "REF**"
		(at -2.2225 24.13 -90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ea31613f-a0a2-4f5a-9373-bee042a054d1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify top)
		)
	)
	(property "Value" "RaspberryPi_Pico_PinSocket_1x20_P2.54mm_Vertical"
		(at 2.54 24.13 90)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "0d39661e-f40b-4a60-8ec8-51a5d8c091da")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify right)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "009a3e96-b8b9-4a7a-9d96-22ce82e98310")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "65295e81-0573-4b70-9c6c-31c8c6541bb8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "de29a954-1bec-4b5c-8476-78d6a7ae56c7")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.38 -0.87)
		(end -1.38 49.13)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "08c81f19-31d3-4dc1-9bec-c63de0a64b46")
	)
	(fp_line
		(start -1.38 1.27)
		(end 1.07052 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2359bd87-7faa-4900-9b5a-8b38a6c995ec")
	)
	(fp_line
		(start 1.38 -1.16)
		(end 1.38 -0.56648)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bc9ec2be-a254-4513-abd6-2044f0da01d1")
	)
	(fp_line
		(start 1.38 1.82648)
		(end 1.38 46.43352)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c49ff0a1-18f8-4276-98ee-73acf4243348")
	)
	(fp_line
		(start 1.38 49.42)
		(end 1.38 48.82648)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e0e18052-83b9-468e-a6c7-19e4c034896d")
	)
	(fp_rect
		(start -1.77 -1.77)
		(end 1.77 50.03)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "bc5efd89-3175-4885-94e9-336f8ced367b")
	)
	(fp_poly
		(pts
			(xy -1.27 -0.635) (xy -0.635 -1.27) (xy 1.27 -1.27) (xy 1.27 49.53) (xy -1.27 49.53)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "ba98a7ec-6ca9-4980-b148-9374515c6ea7")
	)
	(fp_text user "${REFERENCE}"
		(at 0 24.13 90)
		(layer "F.Fab")
		(uuid "f2c62150-a06b-4fb3-87bf-608b0233967d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.125)
		(uuid "a4de5d66-f1a5-4c41-a2c0-35c3c34b7936")
	)
	(pad "2" thru_hole circle
		(at 0 2.54)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a8699681-70f3-46c6-94ea-3faf0b4fff2f")
	)
	(pad "3" thru_hole custom
		(at 0 5.08)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 0.6)
				(end 0.8 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 -0.6)
				(end 0.8 -0.6)
				(width 0)
				(fill yes)
			)
		)
		(uuid "f32146c8-6099-4c07-a87d-a7350676de31")
	)
	(pad "4" thru_hole circle
		(at 0 7.62)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8ce70cbd-2b34-4b6a-b7b5-079884887485")
	)
	(pad "5" thru_hole circle
		(at 0 10.16)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "89630bb3-6203-4757-b039-f5250c28e503")
	)
	(pad "6" thru_hole circle
		(at 0 12.7)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d98a9f0c-b4e9-4c36-a342-3dc6150fb732")
	)
	(pad "7" thru_hole circle
		(at 0 15.24)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ecfbe0aa-79fe-4a73-be7a-59b37d92005e")
	)
	(pad "8" thru_hole custom
		(at 0 17.78)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 0.6)
				(end 0.8 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 -0.6)
				(end 0.8 -0.6)
				(width 0)
				(fill yes)
			)
		)
		(uuid "9900b075-35de-4f2f-8c4a-7d9bd7c9aded")
	)
	(pad "9" thru_hole circle
		(at 0 20.32)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c30140c6-4e71-40f4-ae66-f74946196ab7")
	)
	(pad "10" thru_hole circle
		(at 0 22.86)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "39d694d3-dd15-4333-82ae-91ce5a94d741")
	)
	(pad "11" thru_hole circle
		(at 0 25.4)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "aa9efcfc-8e8d-4eef-aacf-bff36a24b6bc")
	)
	(pad "12" thru_hole circle
		(at 0 27.94)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7f7de844-7fa2-47ff-9e0b-29dcd5a115e5")
	)
	(pad "13" thru_hole custom
		(at 0 30.48)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 0.6)
				(end 0.8 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 -0.6)
				(end 0.8 -0.6)
				(width 0)
				(fill yes)
			)
		)
		(uuid "804e0bba-ccd3-4b8c-babb-1f60cf38cf67")
	)
	(pad "14" thru_hole circle
		(at 0 33.02)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fc23f28e-9244-4c78-bd58-88a2975e72b1")
	)
	(pad "15" thru_hole circle
		(at 0 35.56)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b28a82f8-f314-445b-b63e-ea63506627d7")
	)
	(pad "16" thru_hole circle
		(at 0 38.1)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3433bdb3-efa0-49a8-adcf-46f17f100d85")
	)
	(pad "17" thru_hole circle
		(at 0 40.64)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cb119515-81e1-4cbf-be1f-7d5ad990672c")
	)
	(pad "18" thru_hole custom
		(at 0 43.18)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 0.6)
				(end 0.8 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 -0.6)
				(end 0.8 -0.6)
				(width 0)
				(fill yes)
			)
		)
		(uuid "b4d09f8c-6f88-4977-94f0-851af1eadb7a")
	)
	(pad "19" thru_hole circle
		(at 0 45.72)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fe860644-0583-46d8-9a7e-bd4ccb58e54b")
	)
	(pad "20" thru_hole circle
		(at 0 48.26)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2b48150d-ff7b-4188-bf1c-5ab293a6baa4")
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x20_P2.54mm_Vertical.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "../Module_RaspberryPi_Pico.3dshapes/PinSocket_1x20_H8.51mm_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
