(footprint "RaspberryPi_Pico_OptionalKeepoutRF"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Supplementary RF keepout zone for the Raspberry Pi Pico W (wireless), to be added to other Raspberry Pi Pico footprints, https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf")
	(tags "Raspberry Pi Pico module keepout rf wireless extra addon")
	(property "Reference" "REF**"
		(at 11.7475 24.765 0)
		(unlocked yes)
		(layer "Cmts.User")
		(hide yes)
		(uuid "ea31613f-a0a2-4f5a-9373-bee042a054d1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "RaspberryPi_Pico_OptionalKeepoutRF"
		(at 0 36.195 0)
		(unlocked yes)
		(layer "Cmts.User")
		(hide yes)
		(uuid "0d39661e-f40b-4a60-8ec8-51a5d8c091da")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2d25956e-8c42-41b7-8a9a-f2e0929bed30")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "95525635-6531-4805-ab93-7b59b913fcd9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "ee2ca12c-0ef2-4b7e-b9e3-27e233650de3")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr board_only exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
	(fp_circle
		(center -5.7 23.5)
		(end -4.65 23.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill none)
		(layer "Dwgs.User")
		(uuid "82f31566-8d6b-4211-8754-77aa301d76db")
	)
	(fp_circle
		(center 5.7 23.5)
		(end 6.75 23.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill none)
		(layer "Dwgs.User")
		(uuid "160c447b-6388-48c1-8242-12e3011512bf")
	)
	(fp_text user "2.4 GHz RF Keep Out"
		(at 0 31.75 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "05c13b11-bffb-427b-af67-76d55ef36f21")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "^ Suggested board edge for RF ^"
		(at -14.05 26.67 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "1f07a15d-ab4b-47ce-ac99-1b011e1abd9a")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(fp_text user "^ Suggested board edge for RF ^"
		(at 14.05 26.67 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "378d6a1f-7d98-4c61-96a8-31cd60015d16")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(fp_text user "Keep unobstructed by metal as far as possible in all dimensions"
		(at 0 33.9725 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "8ba7646f-3410-4b7e-9354-9a6e92bc33e9")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(fp_text user "^ Suggested board edge for RF ^"
		(at 0 17.78 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "ad6b2d46-d63f-4d78-a85c-c87399965902")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu" "*.Paste")
		(uuid "ee247754-2270-409a-ad04-c8ac65db609d")
		(name "RF Copper Keep Out")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -21 25) (xy 21 25) (xy 21 35) (xy -21 35)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "Edge.Cuts")
		(uuid "e578e5ea-ecaa-4070-a90d-95a0c77d4f06")
		(name "Board Keep Out Suggestion RF")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 7.1 26) (xy 21 26) (xy 21 35) (xy -21 35) (xy -21 26) (xy -7.1 26) (xy -7.1 17) (xy 7.1 17)
			)
		)
	)
	(group ""
		(uuid "ae46f597-14c9-45f0-bcaf-d5e88c0493c8")
		(members "05c13b11-bffb-427b-af67-76d55ef36f21" "160c447b-6388-48c1-8242-12e3011512bf"
			"1f07a15d-ab4b-47ce-ac99-1b011e1abd9a" "378d6a1f-7d98-4c61-96a8-31cd60015d16"
			"82f31566-8d6b-4211-8754-77aa301d76db" "8ba7646f-3410-4b7e-9354-9a6e92bc33e9"
			"ad6b2d46-d63f-4d78-a85c-c87399965902" "e578e5ea-ecaa-4070-a90d-95a0c77d4f06"
			"ee247754-2270-409a-ad04-c8ac65db609d"
		)
	)
)
