(footprint "RaspberryPi_Pico_OptionalKeepoutUSB"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Supplementary USB cable keepout zone for the Raspberry Pi Pico and Pico W, to be added to other Raspberry Pi Pico footprints")
	(tags "Raspberry Pi Pico module keepout usb plug port cable clearance courtyard extra addon")
	(property "Reference" "REF**"
		(at 6.985 -46.585 0)
		(unlocked yes)
		(layer "Cmts.User")
		(hide yes)
		(uuid "ea31613f-a0a2-4f5a-9373-bee042a054d1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "RaspberryPi_Pico_OptionalKeepoutUSB"
		(at 0 -49.125 0)
		(unlocked yes)
		(layer "Cmts.User")
		(hide yes)
		(uuid "0d39661e-f40b-4a60-8ec8-51a5d8c091da")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 -28.17 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2d25956e-8c42-41b7-8a9a-f2e0929bed30")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 -28.17 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "95525635-6531-4805-ab93-7b59b913fcd9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 -28.17 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "ee2ca12c-0ef2-4b7e-b9e3-27e233650de3")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr board_only exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
	(fp_text user "Keep Out"
		(at 0 -36.195 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "01e7ec74-56c3-42cb-8c5c-95d18439d122")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "USB Cable"
		(at 0 -38.735 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "0f9697f1-fa82-431a-8712-a6fb98ce47d6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "Edge.Cuts")
		(uuid "ad9ab7a0-7945-4719-8203-814a85358df2")
		(name "Board Keep Out USB Cable")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -6.2 -47.65) (xy 6.2 -47.65) (xy 6.2 -27.25) (xy -6.2 -27.25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.CrtYd")
		(uuid "f53c81a9-31a2-4a17-a92e-48e66badd2b1")
		(name "USB Cable Keep Out")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -5.75 -27.7) (xy -3.94 -27.7) (xy -3.94 -27.4) (xy 3.94 -27.4) (xy 3.94 -27.7) (xy 5.75 -27.7)
				(xy 5.75 -47.2) (xy -5.75 -47.2)
			)
		)
	)
	(group ""
		(uuid "823f00c4-a960-4f62-a316-66be0b21ffe7")
		(members "01e7ec74-56c3-42cb-8c5c-95d18439d122" "0f9697f1-fa82-431a-8712-a6fb98ce47d6"
			"ad9ab7a0-7945-4719-8203-814a85358df2" "f53c81a9-31a2-4a17-a92e-48e66badd2b1"
		)
	)
)
